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Wind Turbine/Load Sink Interface Board


Schematic and BOM #1002298


PWB #1002302 "WINDLOAD"





1.	Install CI3/CI4 "DIN Power Contact" in six places provided on connector P3, "DIN_42+6".





2.	Do not install R16, R17 (values TBD at MBARI).





3.	Do not install JMP1, JMP2.





4.	This board uses 2 oz copper.  Please adjust solder profiles accordingly.














