secondary_1481-SBE37SM_1277

1. Manually-configured instrument settings not handled by service

SBE37-SM-PUCK V 1.0-01  SERIAL NO. 2004    01 Jan 1996  02:38:33
logging not started

sample interval = 600 seconds

samplenumber = 0, free = 223914

do not transmit real-time data

do not output salinity with each sample

do not output sound velocity with each sample

store time with each sample

number of samples to average = 4

reference pressure = 0.0 db

serial sync mode disabled

wait time after serial sync sampling = 30 seconds

PUCK mode enabled

internal pump not installed

temperature = 24.45 deg C

SBE37-SM-PUCK V 1.0-01  2004

temperature:  10-jan-06

    8.589752e-05

    2.463458e-04

    -1.457548e-07

    9.862900e-08

conductivity:  10-jan-06

    -9.595624e-01

    1.357190e-01

    -1.282170e-04

    3.166723e-05

    -9.570000e-08

    3.250000e-06

    8.208646e-06

rtc:  10-jan-06

    9.999781e-01

    1.739701e-06

    -3.278540e-08

2. Device metadata returned in SIAM datastream

See (1)

3. Instrument-specific service properties

None

4. Initial service property values for this deployment

powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=org.mbari.isi.interfaces.InstrumentServiceAttributes

serviceName=Seabird-37SM s/n 37SM26805-2004

parentID=1481

currentLimitMa=5000

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

extendedVersion=UNK

frameworkVersion=$Name: march14_2006 $

UUID=211793a6-c3cf-11d9-8c1e-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1277

sampleTimeoutMsec=15000

commPowerPolicy=SAMPLING

serviceStatus=0

startDelayMsec=2000

5. Results of acceptance test procedures

All passed

6. Known-service bugs/deficiencies

unable to access XML file

Instrument internal clock not set







