Instrument name here

1. Commands issued by service at initialization 



disableAllNMEA();



setNMEAMessage("GPRMC,1");



setNMEAMessage("GPGSV,1");



setNMEAMessage("PGRMT,1");
2. Commands issued by service for safe mode, if applicable
N/A
3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.garmin.GarminGPS$Attributes

serviceName=Garmin GPS s/n 81106809

parentID=1481

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

defaultSkipInterval=0

fixTimeoutMsec=900000

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=a36ed0b8-8dd5-11da-92c6-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=15

isiID=1504

peakCurrentMa=5000

summaryTriggerCount=0

sampleTimeoutMsec=10000

commPowerPolicy=SAMPLING

serviceStatus=2

startDelayMsec=2000

isiID = 1504

serviceName = Garmin GPS s/n 81106809

powerPolicy = always

commPowerPolicy = sampling

sampleSchedule = 600

currentLimitMa = 3000

UUID = a36ed0b8-8dd5-11da-92c6-00306e389969

$PGRMC,A,55.3,100,,,,,,A,3,1,1,4,30*63

$PGRMC,A,55.2,100,,,,,,A,3,1,1,4,30*62
4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
OK
7. Known-service bugs/deficiencies

None






