Instrument name here

1. Commands issued by service at initialization 

None
2. Commands issued by service for safe mode, if applicable
None
3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.seahorse.Seahorse$Attributes

serviceName=Seahorse Profiler s/n 10322

parentID=1481

maxSummarySamples=0

currentLimitMa=4000

sampleMarginSecs=15

packetSetSize=10

profilerSamplePeriodSecs=14400

sampleSchedule=R */0 */0 */4 */0 * * * * GMT *

defaultSkipInterval=0

extendedVersion=UNK

syncMarginSecs=10

frameworkVersion=$Name: june05_2006 $

errCacheLimit=5

UUID=9751E3A2-94EA-49D1-A1C3-858588C8B74C

signalLine=CTS

powerPolicy=SAMPLING

timeSynch=false

missingFileCount=-24

maxSampleTries=1

radioOnTimeSecs=120

isiID=1405

persistFiles=false

peakCurrentMa=5000

summaryTriggerCount=0

sampleTimeoutMsec=6000

commPowerPolicy=SAMPLING

syncRetryPeriods=2

serviceStatus=2

startDelayMsec=0

isiID = 1405

serviceName = Seahorse Profiler s/n 10322

powerPolicy = sampling

commPowerPolicy = sampling

sampleSchedule = 14400

currentLimitMa = 4000

signalLine = CTS

persistFiles = false

radioOnTimeSecs = 120

profilerSamplePeriodSecs = 14400

syncMarginSecs = 10

sampleMarginSecs = 15

syncRetryPeriods = 2

missingFileCount = -24

UUID = 9751E3A2-94EA-49D1-A1C3-858588C8B74C

Seahorse Profiler s/n 10322 does not provide instrument state information

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
7. Known-service bugs/deficiencies

Leaves files on node;

all files not transferred to shore






