Instrument name here

1. Commands issued by service at initialization 


    _toDevice.write("APP\r".getBytes());


    getInstrumentAttention(3);// "ECHO OFF\r".,”\r”
2. Commands issued by service for safe mode, if applicable
N/A
3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.serialadc.SerialAdc$Attributes

captureParams=ADC BP

serviceName=400-12V Switch s/n 1.02

parentID=1520

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

defaultSkipInterval=0

statusMinSamples=10

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=69712280-ea7b-11da-9cb2-00306e389969

powerWarningLow=11.0

powerPolicy=NEVER

timeSynch=false

powerOkLow=12.0

maxSampleTries=3

isiID=1554

powerStatusChannel=ADC10

peakCurrentMa=5000

summaryTriggerCount=0

dataCountCheck=true

sampleTimeoutMsec=5000

commPowerPolicy=SAMPLING

serviceStatus=2

logTimeSync=true

startDelayMsec=10000

isiID = 1554

serviceName = 400-12V Switch s/n 1.02

powerPolicy = never

commPowerPolicy = sampling

sampleSchedule = 600

captureParams = ADC BP

dataCountCheck = true

logTimeSync = true

powerStatusChannel = ADC10

powerWarningLow=11.0

powerOkLow=12.0

statusMinSamples = 10

currentLimitMa = 3000

sampleTimeoutMsec=15000

UUID = 69712280-ea7b-11da-9cb2-00306e389969

VERSION:

MOOS POWER SYSTEM DAQ 0.7

built on May  9 2006 at 21:57:13

CVS tag "$Name:  $"

CONFIGURATION:

ADC00 S09 C01 P0001000 T0000000 D0 L0 A1

ADC01 S09 C02 P0000250 T0000000 D0 L0 A1

ADC02 S09 C03 P0000250 T0000000 D0 L0 A1

ADC03 S09 C04 P0000250 T0000000 D0 L0 A1

ADC04 S09 C05 P0000250 T0000000 D0 L0 A1

ADC05 S09 C06 P0000250 T0000000 D0 L0 A1

ADC10 S10 C01 P0001000 T0000000 D0 L0 A1

ADC11 S10 C02 P0000250 T0000000 D0 L0 A1

ADC12 S10 C03 P0001000 T0000000 D0 L0 A1

ADC13 S10 C04 P0001000 T0000000 D0 L0 A1

ADC14 S10 C05 P0001000 T0000000 D0 L0 A1

DO00 S-1 C-1 E0000000 D0000000  O0 A1

BP00 S09 C07 P0000250 A1

CALIBRATION:

S09 C01 G+1.5157e-02 O+0.0000e+00

S09 C02 G+7.3240e-06 O+0.0000e+00

S09 C03 G+7.3240e-06 O+0.0000e+00

S09 C04 G+1.1100e-05 O+0.0000e+00

S09 C05 G+1.1100e-05 O+0.0000e+00

S09 C06 G+1.1100e-05 O+0.0000e+00

S10 C01 G+5.6400e-04 O+0.0000e+00

S10 C02 G+4.5780e-04 O+0.0000e+00

S10 C03 G+5.6400e-04 O+0.0000e+00

S10 C04 G+5.6400e-04 O+0.0000e+00

S10 C05 G+2.0220e-01 O-2.7315e+02

CALIBRATION REV "$Revision: 1.13 $"

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
N/A
7. Known-service bugs/deficiencies

Issues “EXIT\r” on shutdown instrument (stops P2 app)






