Instrument name here

1. Commands issued by service at initialization 



disableAllNMEA();



setNMEAMessage("GPRMC,1");



setNMEAMessage("GPGSV,1");



setNMEAMessage("PGRMT,1");
2. Commands issued by service for safe mode, if applicable
N/A

3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.garmin.GarminGPS$Attributes

serviceName=Garmin GPS s/n 81108654

parentID=1446

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

defaultSkipInterval=0

fixTimeoutMsec=900000

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=5db626e7-8dd5-11da-92c6-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=15

isiID=1503

peakCurrentMa=5000

summaryTriggerCount=0

sampleTimeoutMsec=10000

commPowerPolicy=SAMPLING

serviceStatus=2

startDelayMsec=2000

isiID = 1503

serviceName = Garmin GPS s/n 81108654

powerPolicy = always

commPowerPolicy = sampling

sampleSchedule = 600

currentLimitMa = 3000

UUID = 5db626e7-8dd5-11da-92c6-00306e389969

$PGRMC,A,-19.1,100,,,,,,A,3,1,1,4,30*44

$PGRMC,A,-19.1,100,,,,,,A,3,1,1,4,30*44

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
OK

7. Known-service bugs/deficiencies

None






