Instrument name here

1. Commands issued by service at initialization 


_toDevice.write("set echo off\n".getBytes());
2. Commands issued by service for safe mode, if applicable

N/A

3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=moos.devices.msp430.MSP430$Attributes

serviceName=MSP430 (sidearm4.25)

parentID=1446

maxSummarySamples=0

currentLimitMa=3000

turnsSetpoint=0

packetSetSize=10

sampleSchedule=R */0 */10 */0 */0 * * * * GMT *

setTurns=false

defaultSkipInterval=0

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=a92f763a-29ff-11da-80c8-00306e389969

powerPolicy=ALWAYS

timeSynch=false

maxSampleTries=3

isiID=1447

peakCurrentMa=5000

summaryTriggerCount=0

sampleTimeoutMsec=10000

commPowerPolicy=ALWAYS

serviceStatus=2

startDelayMsec=500

isiID = 1447

serviceName = MSP430 (sidearm4.25)

currentLimitMa = 3000

sampleSchedule = 600

UUID = a92f763a-29ff-11da-80c8-00306e389969

$PSID, V2.3.1-Q [Mar 12 2004], *1811

$PALEVEL, PL0.000000, PH0.000000, TL0.000000, TH0.000000, HL0.000000, HH0.000000, GFLL0.000000, GFLH0.000000, GFHL0.000000, GFHH0.000000, CL0.000000, CH0.000000, TCL0.000000, TCH0.000000, *984

$PAMASK, 00, *729

$PALARM, 00, *729

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
N/A

7. Known-service bugs/deficiencies

none






