Instrument name here

1. Commands issued by service at initialization 


// First reset the Medusa


_toDevice.write(CMD_RESET.getBytes()); //! currently given as “meta\r”!


_toDevice.flush();


Thread.sleep(RESET_MSEC);


getPrompt(); //"\r\n"

// Disable command echo


_toDevice.write(DISABLE_ECHO); // "echo n\r\n"

// Send host IP address to Medusa


try {


    InetAddress host = InetAddress.getLocalHost();


    _toDevice.write((SET_IP_ADDRESS + " " + 




     host.getHostAddress() + ENTER).getBytes()); // "saipset"…”/r/n”

}

2. Commands issued by service for safe mode, if applicable

N/A

3. Device metadata returned in SIAM datastream
powerOnDelaySec=0

instrumentName=UNKNOWN

nominalCurrentMa=1000

className=org.mbari.isi.interfaces.InstrumentServiceAttributes

serviceName=Medusa card s/n 2.007

parentID=1446

maxSummarySamples=0

currentLimitMa=3000

packetSetSize=10

sampleSchedule=R */0 */5 */0 */0 * * * * GMT *

defaultSkipInterval=0

extendedVersion=UNK

frameworkVersion=$Name: june09_2006 $

errCacheLimit=5

UUID=e052be35-e4db-11d9-b8bc-00306e389969

powerPolicy=NEVER

timeSynch=false

maxSampleTries=3

isiID=1441

peakCurrentMa=5000

summaryTriggerCount=0

sampleTimeoutMsec=1000

commPowerPolicy=NEVER

serviceStatus=2

startDelayMsec=2000

isiID = 1441

serviceName = Medusa card s/n 2.007

currentLimitMa = 3000

UUID = e052be35-e4db-11d9-b8bc-00306e389969

META:

CPU MAC address: 00:0c:6a:01:02:07

CPU IP address: 134.89.36.57

CPU IP netmask: 255.255.0.0

CPU IP gateway: 134.89.36.200

SideARM IP address: 134.89.36.200

Medusa serial number: 2.007

Medusa ECO level: B

Firmware build: v2.50 [May 17 2006 11:00:10]

Toolchain: Rowley gcc 3.4.4

Trunk Failovers: 10 0

Backplane wakeup interrupts: 10

PORTS:

Port   Status   PHY Stat  Optical   LHB Stat  Last Evt  Fail  LHB OK

F  0    down    pwr save  pwr off   disabled  LHB FAIL     0     0

F  1     up      normal    normal   enabled   LHB FAIL    58     0

F  2     up      normal   unknown   disabled  port up      0     0

F  3  unknown   pwr save  pwr off   disabled  no event     0     0

C  4     up      normal      ---    disabled  no event     0     0

C  5     up      normal      ---    disabled  port up      0     0

NVSHOW:

nvshow: sig[cf] ver[01] firstItemPg[1] numItem[16]

nvshow: firstDataPg[17] numData[16] configCrc16[f9b2]

Item  0 [macaddr]:
0000: 00 0c 6a 01 02 07 

Item  1 [ipaddr]:
0000: 86 59 24 39 

Item  2 [gateway]:
0000: 86 59 24 c8 

Item  3 [netmask]:
0000: ff ff 00 00 

Item  4 [saipaddr]:
0000: 86 59 24 c8 

Item  5 [serial]:
0000: 32 2e 30 30 37 

Item  6 [ecolevel]:
0000: 42 

Item  7 [trunk0]:
0000: 01 00 01 03 

Item  8 [port0]:
0000: 09 

Item  9 [port1]:
0000: 09

UIPSTAT:

uipstat: IP Packets Rx[10] Tx[0] Drop[0]

uipstat: ICMP Packets Rx[0] Tx[0] Drop[0]

uipstat: TCP Packets Rx[0] Tx[0] Drop[0]

uipstat: TCP Packets Retrans[0] Conn Attempts[0]

EVENT:

event: Zarlink events[2621] rxFrame[23] ctrl1[2598] ctrl2[0] reset[0]

U0STAT:

u0stat: maxTx[256] maxRx[1] maxIsrPass[1]

u0stat: txDrop[0] rxDrop[0] spurInt[0] lsrInt[0]

SFPDIAG:

channel=1, temp=49.34, vcc=3.2192, txBiasI=2.8868, txPower=-1.7658, rxPower=-42.4551, status=0x2

channel=2, temp=53.55, vcc=3.2180, txBiasI=3.9969, txPower=-2.6577, rxPower=-9.7832, status=0x0

SHOWSTATS[0]:

--- Zarlink port stats for port [0] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[327680]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

SHOWSTATS[1]:

--- Zarlink port stats for port [1] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[393216]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

SHOWSTATS[2]:

--- Zarlink port stats for port [2] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[0]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

SHOWSTATS[3]:

--- Zarlink port stats for port [3] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[0]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

SHOWSTATS[4]:

--- Zarlink port stats for port [4] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[0]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

SHOWSTATS[5]:

--- Zarlink port stats for port [5] ---

  TX: bytes[0 0]  unicastFrame[0]  frameTxFail[0]

  RX: bytes[0 0]  frames[0 0]  totalBytes[0 0]  totalFrames[0]

  RX: mcastFrames[0]  bcastFrames[0]  flowCtrlFrames[0]

 ERR: align[0]  runt[0]  crc[0]  shortEvent[0]

FLOW: flowCtrlFramesRecv[0]  flowCtrlSent[0]

 PKT: len64[0]  len65-127[0]  jabber[0]  oversize[0]

 LEN: 128-255[0]  256-511[0]  512-1023[0]  1024-1522[0]

OOPS: fragment[0]  dropped[0]  filterCount[0]  delayExceedDiscard[0]

4. Instrument-specific service properties
5. Initial service property values for this deployment
6. Results of acceptance test procedures
OK

7. Known-service bugs/deficiencies

The reset command may be incorrect (currently “meta” should be “reset”)






