


How long to try to wake subnodes


Timeouts for successful shutdown








Get list of downstream nodes (not the same as SIAM subnodes)





Wait for notification from downstream nodes





Terminate Local Instrument Services (except P2 service)








Get Local P2 


Service Proxy








Set Power Backups


Disable for full shutdown


Enable for safe shutdown








How to discover power topology


Property of P2 service?


Property of node service?


level number?








How to exclude shutdown for P2 service?


How to manage P2 power (on SR port)?





Exit local SIAM Application








Sync local filesystem








Halt Sidearm








How to Sync/Halt system w/o SIAM? W/o network?


Do locally? Remotely?


Software Watchdog?


Time delay script/cron task?


Server/driver in linux?








Notify upstream node (power parent): shutdown   complete








Initiate Shutdown


For downstream nodes





Shut down HV to downstream nodes








Initiate Shutdown (full/safemode)





Put instruments into safe mode (safe shutdown)








Initiate Shutdown any remaining nodes (mis-numbered)





Inefficient to rediscover subnodes at each level


Recursive or Top Down?


Discover once, call this.level+1, passing  topo info down?








How to notify w/o network?





Wait for notification from downstream nodes





What to do about unknown nodes or nodes that won’t wake up





Must shutdown/safemode instruments before disabling power backups (Instruments needing holdup caps may sample after they are disabled)








