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Mooring Buoy Controller System

Detailed Engineering Requirements

Revision: 1.0

Shore-link Interface:

· In the event of a ground fault, must be isolatable without affecting the rest of the system.  

· Must be able to disable and isolate the link and have it automatically reestablish the link after a short period of time (_____ seconds).  

· Must provide a data bandwidth of at least _________ bps

· Must use a maximum of _______A at ________V (____5?___W) when transmitting

· Must use a maximum of _______A at ________V (_________W)  when not transmitting

