1. Check the strain gauge power supply to ensure it's still operational

2. Update the heave sensor driver with the correct sampling time

3. Check the sidekick ground fault

4. Check the sidekick humidity sensor

5. Double check ARGOS data transmissions (it looked like it hung up before we recovered it.)

6. Upper bending strain relief needs to be redesigned/replaced

7. recover Power Can to lab; investigate current sensor interaction

8. open Load Dump Box, check condition of load dump resistors 

9. check entire system for ground faults

10. visually inspect all cabling for chafe and wear

Optional:

11. Change driver data formats to make it easier to automatically produce (plottable, printable, browseable) netCDF files

12. Update controller can SmartStar driver and firmware to the same that's running in the power can

