VERTICAL PROFILER CALCULATIONS

GIVEN:
Instrument package weight in water = xlbs
Operating depth = 60 FT

FIND:
Force of drag on system
velocity of system

Specific Wt. of AIR

Density of Sea Water

Coefficient of Drag

SPECIFIC WEIGHT WATER

Diameter

Area

SPECIFIC WT FLUID/SOLID

Viscosity of Sea water

Terminal Velocity
from drag equation
Terminal Velocity
with x lbs force

Reynolds Number