TIBURON DRILL SLED 

ASSEMBLY PLAN 

· SECURE ALL NECESSARY PICTURES, DRAWINGS AND DOC’S

· REMOVE AND MODIFY EXISTING DRILL FRAME STRONGBACK.  COMPRISING THREE PLATES.  FINISH: HARD BLACK ANODIZDE  per MIL-A-8625F TYPE III

· INSTALL FRAME INTO TOOL SLED SUCH THAT THE DRILL STRING IS ON CENTERLINE BOTH VERTICALLY AND HORIZONTALLY.  INSALL FORWARD, CENTER, AND AFT BRACKETS.  MATCH DRILL HOLES TO FRAME.

· INSTALL CUTTER FRAME ALIGNED WITH THE DRILL STRING.  MATCH DRILL BRACKET HOLES TO FRAME.

· INSTALL VALVE PACK, WATER PUMP, AND DECONN.  POSITIONS TO BALANCE THE WEIGHT.

· ROUTE AND INSTALL HYDRAULIC TUBES AND HOSES TO MATCH NEW HYDRAULIC CIRCUIT DIAGRAM.

· ROUTE AND INSTALL ALL WIRING

