Environmental Sample Processor

June 28, 2000

PUNCH LIST

· ESP- (formerly known as Genosensor)

1. Install Button assembly & ULS on load elevator. 

2. Replace plastic support rods with aluminum

3. External floatation and brackets for Housing

4. Internal Mount for Bag’s

5. Surface float

6. Float

7. Antenna tower

8. Pot e/m terminations

9. Build e/c wire seal mold

10. Build up surface float

11. Battery pack: Mount stand-offs to Batt-Pack and assemble to lower Endcap.

12. Transport deployment box

13. Mold new heater pads (18.6 Ohm heaters)

14. Clamp Assembly mods

15. better strain relief

16. bigger wire slot

17. new coupling

18. heater spacer for molding process

