DORISS 2 Focus Stage Motor Set-up
(1) Begin by moving the motor in the positive direction until the “Limit 1” switch is reached. The maximum motor count (and the range of motion in motor counts) is approximately 804,200. The positive direction is away from the glass dome.

(2) After the “Limit 1” switch is reached, back away from the switch 2,100 counts for a safety margin. Example: after reaching the Limit 1 switch, the motor position reads 245,210. Entering 243,110 into the desired position field (upper right corner of the dialog) and pressing the “Go” button will back the motor up an adequate safety margin (do NOT move more than 2500 counts away from Limit 1).

(3) After backing away to the margin, you want that position to be the limit that the GUI will allow you to move in the positive direction. In order to tell the GUI that the motor is in that position, you will enter the number “771907734” into the desired position field (that number is “hELLObILL” upside down). The GUI will reset it’s current position to be 800,000 counts. Now, the allowable range of motion is set from 0 to 800,000.

(4) To reset the limit positions, you will need to turn the software limits off. This is done by entering the number “90907734” (upside down “hELLObOb”). The motor will then be able to move beyond 0 and 800,000 but you can damage the hardware if you are not careful.
