DORISS/PUP System Test Checklist

Communications check:  From a CMD window…


Check Mudpuppy (or Ramandesktop)
C:\> ping mudpuppy



IP address should be 134.89.10.93 (or 134.89.10.92)


Check Galil (134.89.10.96)
C:\> ping galil


Check Axis Server (134.89.10.95)
C:\> ping axis

PUP GUI check:

Double-click on PUP.exe icon to start PUP GUI

Check all features

· Make sure axes position numbers look reasonable

· Make sure tilt, temperature, humidity numbers look reasonable

· Turn camera on

· Double-click on Internet Explorer and check camera output

· Turn lasers on and off

· Turn light on and off

· Turn camera off

Check positioning

· Jog all three axes in both the positive and negative directions

· Run Homing command (double click on the button)

· Make sure the axes’ positions decrease and set to zero 

· (homing completed when error numbers are ~0)

· Go to HOME position

DORISS check:

Turn on DORISS the the button on the PUP GUI 

Check Ramansbc from a CMD window



C:\> ping ramansbc or doriss


IP address should be 134.89.10.94  (It takes 2 minutes to fully boot up.)

Open LRSClient on the host computer


 (should take a few minutes, click Ignore for any error message)

Open VNC and login to ramansbc (IP address: 134.89.10.94,  password: LRS)

· Verify that temperature & humidity date are scrolling in one of the CMD windows

Open HoloGRAMS by double-clicking on the HoloGRAMS icon on the host computer


(I2C error is normal)

· In Acquire tab, set exposure to 1 sec, click Focus button (may have to hit button again).

· Verify that spectrum refreshes every second.

· Stop Focus mode and exit HoloGRAMS

After checking all features, exit everything except for VNC.  

On ramansbc desktop select Shutdown – turn off DORISS (from PUP GUI) after 35 sec.

