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LRS Operations Overview

Power ON host computer:
Ramandesktop
User
Administrator


Password
LRS


Mudpuppy
User
puppy



Password
puppy
Power ON LRS (Takes 2 minutes for Ramansbc to complete full boot up)

Use Ping to verify connection from host to Ramansbc

On Mudpuppy/Ramandesktop:


In command window
ping –t ramansbc
Use HoloGRAMS to collect spectra  (See HoloGRAMS manual for operational information)


HoloGRAMS shortcut on Ramandesktop desktop

Use PCAnywhere/VNC/NetMeeting to monitor sensor data and operate remote stages


PCAnywhere/VNC/NetMeeting shortcut on Ramandesktop desktop or taskbar


User
Administrator

Password
LRS

There should be five windows open on the Ramansbc desktop:



AT Server



client



C:\winnt\System32\CMD.exe

(one of these will have scrolling



C:\winnt\System32\CMD.exe


temp and humidity data)



C:\winnt\System32\CMD.exe
NOTE:  Do NOT close windows on Ramansbc desktop, only minimize them


Use LRSClient to monitor temperature, humidity and water alarm



runclient shortcut on Ramansbc desktop (executable in C:\LRS App\ )



LRSClient takes about a minute to come up



NOTE:  LRSClient window must be open to see water alarm


Use MVPdemo to run slit and focus stages  (see MVP manual and cheat sheet)



mvpdemo shortcut on Ramansbc desktop 

(executable in C:\program files\National Aperture’s Mvpdemo\ )

To Shutdown, on Ramansbc:

Start ( Shut_Down
Wait 30-40 seconds then power OFF LRS
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