DORISS/PUP Network Configurations

POINT-TO-POINT with fixed IP Addresses for MBARI Bldg. A Network


Ramandesktop
134.89.10.92
ramandesktop

Mudpuppy
134.89.10.93
mudpuppy

DORISS (LRS) 
134.89.10.94
ramansbc  or  doriss

Axis Video Server (PUP)
134.89.10.95
axis

Galil Controller (PUP)
134.89.10.96
galil
Network configuration settings for host computer (i.e. ramandesktop or mudpuppy)

Internet Protocol (TCP/IP) Properties


General Tab:



Subnet Mask:
255.255.254.0



Default Gateway:
134.89.10.1



DNS Enabled
(


DNS Servers:
134.89.10.26




134.89.10.17


Advanced Settings:


WINS



WINS Addresses:
134.89.10.32




134.89.12.87



Enable NetBIOS over TCP/IP  (
System Properties


Network Identification



Domain:
LAGOON

Miscellaneous Info

Axis Video Server Address is 00-40-8C-5E-AD-72

Galil Controller settings are…


Controller 1
DMC-2100
Timeout = 5000


TCP
Use current “CF” settings

