DORISS/PUP Pre-cruise Tasks

C-9 days
Test DORISS & PUP before assembling inside housings



[2 team members]

C-8 days
Seal housings; clean and connect all cables; vacuum check housings overnight



[2 team members]

C-7 days
Test DORISS/PUP in the lab, both separately and together (calibrate DORISS)



[2 team members]

C-6 days
Test DORISS/PUP in the lab, both separately and together



[2 team members]

C-5 days
Test DORISS/PUP in test tank



[2 team members]

C-4 days
Test DORISS/PUP in cold room (calibrate DORISS)



[2 team members]

C-3 days
Work on cruise configuration of DORISS/PUP



[ME, science team, techs]

C-2 days
Work on cruise configuration of DORISS/PUP



[ME, science team, techs]

C-1 days
MOB day.  Load DORISS/PUP on ship; integrate with ROV; test



[full team]

Cruise Day
Arrive at ship at designated time; test DORISS/PUP on transit to site



[full team]

For instructions on assembling DORISS in housings (see LRS Assembly Check List).

Instructions for sealing the PUP sphere are listed on sphere.

Key assembly tasks include:

· Clean all sealing surfaces; clean and grease all o-rings

· Clean, check and grease all o-rings in cable connectors

· Connect laser cable to electronics housing and check laser power

· Close up all housings (put desiccant in all housings)

· Connect all cables

· Check all swagelok fittings

· Vacuum check housings

For Testing instructions see DORISS/PUP System Test Checklist

