FROM: Mark Brown

MBARI

7700 SANDHOLDT RD.

MOSS LANDING CA 95039

PH: 831 775-1939

Fiber Optic Cable termination instructions

1-Blue Polyurethane cable assembly:

Remove existing fiber optic ST connectors and replace with 50/125um FC connectors provided.

2-Black Polyurethane cable assembly:

Remove existing fiber optic ST connectors and replace with 100/140um FC connectors provided.

3-Threaded Port Connector assembly: (2ea -black jacket FO)

Remove existing fiber optic ST connectors and replace with 50/125um FC connectors provided.

4- Threaded Port Connector assembly: (1ea.-Orange jacket FO)

Remove existing fiber optic ST connectors and replace with 100/140um FC connectors provided.

