Boundary Condition Testing

(In Air)

The following is a set of tasks that should be completed before the dive deployment in late August.

· Repeat deflection testing at 1cm increments using actual Probe Head Assembly.

· Develop Boundary Condition Test Plan.

· Complete Boundary testing for laboratory use of probe head assembly IN AIR. This testing should be completed before paper submittal July 15?

· Hydrostatic test of glass instrument housing.

· Hydrostatic test of actuator assembly.

