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Precision Underwater Positioner Test Plan

Sub-System Testing – Visualization System

Camera – Field of view [Sec 2.5.1 (3)]
Rev 1.0


Date: 

Testers: 

Temp: 

Location: 

Air/Water

Orientation:  vertical / horizontal

Camera-Target Distance (cm)
Frame Grab File Name
Image Height
Image Width
FOV (vertical)
FOV (horizontal)
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