2 Sub-System Testing

2.1 Actuation

The purpose of these tests is, to confirm correct operation of the actuators used on PUP.   These tests may be used on or off the PUP for confirmation of operation.

2.1.1 Required Equipment

1) Galil motor controller

2) Actuator

3) AMC servo amp DR100RE30A40NDC

4) Power Supply PS30A-LV

5) 12” Ruler 

6) 0 - 50oC water bath

7) 0 - 50oC environmental chamber

2.1.2 Caution

This test involves high DC and AC voltages.  Care must be taken in the setup and execution of this procedure.  As water is involved appropriate measures must be taken to ensure adequate grounding and personnel protection.

2.1.3 Testing procedure for Z, and R Axis
1) Limits Of Travel

Description: This test has three purposes, 1) Limit switch operation, 2) distance of travel and, 3) fully retracted shaft extension.

Definition of Terms: 

RESOLUTION; The smallest position increment achievable. For the PUP the specification for resolution = .1mm

ACCURACY; The maximum error between expected or input and actual position.

REPEATABILITY; The measure of accuracy when returning to a given point after moving.

Setup: Configure AMC to Drive Servo, connect the Galil controller and Power Supply and Servo to AMC servo AMP.  

Procedure: Jog servo in the retract direction until Limit switch is activated.  Measure from Servo housing to base of thread on the ram.  Mark this location for comparison to fully extended position.  Jog servo in the extend direction until the other Limit Switch is activated.  Measure distance between activation points.

Recorded information: Retract and Extend Limit switch Pass/Fail, Servo counts at fully retracted and extended positions, delta of 89600 (2560, and Distance traveled 8.75” (0.25”.  In fully retracted position, distance from servo housing to the base of thread on the ram 1.0” (XXX.  (Mark need numbers)

2) Home Limit Repeatability

Definition: The test is to ensure the limit switch in the retract position has an acceptable repeatability.

Setup: Configure AMC to Drive Servo, connect the Galil controller and Power Supply and Servo to AMC servo AMP.  

Procedure: 

1) Jog servo, in the retract direction, at a velocity of 1024 count/second until Limit switch is activated.

2) Reset Servo counts, and measure position relative to housing.

3) Extend servo 5000 counts.

4) Jog servo, in the retract direction,  at a velocity of 100 counts/second until Limit switch is activated.

5) Measure position relative to housing and record counts.

6) Repeat 3,4,5 2 more times.

Recorded Information: record at each limit switch activation 1) counts and, 2) distance from housing to base of thread on ram.  Calculate delta from first measurement to others, delta less than (0.5mm.  

3) Position Resolution

Definition: The purpose of these tests is to determine the positioning accuracy of the Servo.  Relative, absolute and repeatability will be determined.

Set up: Configure AMC to Drive Servo, connect the Galil controller and Power Supply and Servo to AMC servo AMP.  

Procedure: After the actuator is “homed”, follow these steups:

1) Measure and record from housing to base of ram thread.

2) Move actuator 10240 counts out

3) Repeat 1,2 for seven steps.

4) Home actuator

5) Repeat 1,2,3 for 3 cycles.

6) Move actuator 10240 counts in

7) Measure and record from housing to base of ram thread.

8) Repeat 6,7 for seven steps

9) Move actuator to absolute position 81920.

10) Repeat 7,8,9 for 3 cycles.

11) Move actuator to absolute position 40960.

12) Measure ram position.

13) Move actuator 40 counts out.

14) Measure ram position.

15) Move actuator 40 counts in.

16) Measure ram position.

17) Repeat 12-16 for 3 cycles.

Recorded Information: All information measured in procedure.  Measurements in step 1-10 shall be at 25.4 (1mm increments.  Measurements at steps 13 and 15 shall be a delta of 0.1 (XXXmm.   (need Mark’s input)

4) Temperture

Repeat all tests above with the actuator at 0 and 50​oC. 
5) Water

Repeat all tests above with actuator submerged in water at temperatures of 0 and 50(5(C. 

6) Pressure

Repeat all tests above with actuator at 6000 (XXX PSI and at temperatures from 0 to 50(5(C.

2.1.4 Other Axis
TBD based on design.
2.2 Power System

This section will be to test the main power system of the PUP.  Since the PUP is supplied by 2 sources, 240VDC and 110VAC two different test sections will be required.  The first section will test each of the items, which draw power.  This test will be carried out with a 100VAC 60Hz source single phase as the source, as this is PUP’s primary power source.

2.2.1 110VAC source

2.2.1.1  Caution

This test involves high AC voltages.  Care must be taken in the setup and execution of this procedure.  As water is involved appropriate measures must be taken to ensure adequate grounding and personnel protection.

2.2.1.2 Equipment required

1) Power source

a) Nominal 110VAC, variable from 110 to 130VACrms

b) 60Hz

c) 1VA

2) Oven capable of 0-50(C

3) RMS meter

4) DC voltage meter capable of reading 200VDC minimum.

5) DC current meter capable of measuring up to 20 amps.

6) Power loads as specified within subsection.

7) Oscilliscope

Isolated probe ground from power neutral

Capable of over (200VDC on input

2.2.1.3 Servo Power supply (PS30A-LV)

Definition: this procedure will be used to determine the accetablility of the servo power supply.  This test will check out not only the main power handling but the regenrative braking load.  This test will not be preformed in water as this sub-system is housed within the main PUP glass ball, and will be assumed this will be a sealed environment.

Setup:  This test will require resistive power loads as follows:

1) 30K( at 1Watt,

2) 3K( at 10Watts,

3) 240( at 50Watts.

This test will also require a high voltage DC power supply capable of supplying 200V at 100ma.

Test procedure:  The following steps will be to confirm the conversion capability of the power supply.

1) Ensure AC power source is OFF.

2) Connect AC power source to C1 pins AC1 and AC2 of the PS30A-LV.

3) Connect load, per table, across power supply out, Power Gnd to High Voltage

4) Turn AC power source ON.

5) Set AC RMS voltage to value specified in table

6) Verify Regen green LED on Power supply is solid on

7) Measure RMS output Voltage

8) Using Oscilliscope Measure ripple voltage 

9) Turn AC source OFF

10) Repeat steps 3-9 for all loads and voltages in table

The following procedures will be use to test the Regenarative breaking function

11) Disconnect AC power source from PS30A-LV.

12) Install jumper between pins 4 and 5 of C2.

13) Connect High Voltage DC power source to the power supply output, Power Gnd to High Voltage

14) Turn Power Supply on and ramp Dc output voltage up till the Regenerative Braking LED begins to flash.

15) Measure the applied DC voltage.

AC input (Vrms)
Load (()
RMS output (V)
Ripple

110
30K
155(5%


110
3K
155(5%


110
240
155(5%


124
30K
175(5%


124
3K
175(5%


124
240
175(5%


130
30K
185(5%


130
3K
185(5%


130
240
185(5%







16) Perform the above test sequence in a thermal chamber with the ambient temperature set to 0 and then at 50(C.

Recorded information: Record the RMS output voltage at each step in the table.  Record the Regenerative breaking voltage.

2.2.1.4 12V Power Supply (NLP25-7612)

Definition: The purpose of this test is to verify the functionality of the PUP’s 12 volt power supply.

Setup: This test will require resistive power loads as follows:

1) 12( at 12 Watt,

2) 24( at 6 Watts.

Test Procedure: Follow this procedure to complete test:

1) Ensure AC power source is OFF

2) Connect AC power source to J1 pins 3 and 5 of the NLP25-7612.

3) Connect load, per table, across power supply out,  J2 pin 1 and 2.

4) Turn AC power source ON.

5) Set AC RMS voltage to value specified in table

6) Measure RMS output Voltage

7) Using Oscilliscope Measure ripple voltage 

8) Turn AC source OFF

9) Repeat steps 3-8 for all loads and voltages in table

AC input (Vrms)
Load (()
RMS output (V)
Ripple

110
12
12(2%


110
24
12(2%


124
12
12(2%


124
24
12(2%


130
12
12(2%


130
24
12(2%


Recorded information:  Record the output voltage and ripple voltage at each load input voltage combination.

2.2.1.5 24 Volt Power Supply (NLP….)

The purpose of this test is to verify the functionality of the PUP’s 24 volt power supply.

Setup: This test will require resistive power loads as follows:

3) ??( at ?? Watt,

4) ??( at ?? Watts.

Test Procedure: Follow this procedure to complete test:

10) Ensure AC power source is OFF

11) Connect AC power source to J1 pins 3 and 5 of the NLP…..

12) Connect load, per table, across power supply out,  J2 pin 1 and 2.

13) Turn AC power source ON.

14) Set AC RMS voltage to value specified in table

15) Measure RMS output Voltage

16) Using Oscilliscope Measure ripple voltage 

17) Turn AC source OFF

18) Repeat steps 3-8 for all loads and voltages in table

AC input (Vrms)
Load (()
RMS output (V)
Ripple

110
12
12(2%


110
24
12(2%


124
12
12(2%


124
24
12(2%


130
12
12(2%


130
24
12(2%


Recorded information:  Record the output voltage and ripple voltage at each load input voltage combination.

2.2.1.6 Camera Light

Definition:   The purpose of this test is to check functionality of the camera light.  This light is a 110V 100watt incandescent light.

Setup:  Connect Light using cable and extra connector.  From this connecotr wire in a series a Ammeter.  And finally connect to AC source.

Procedure: Set Ac source to 110VAC RMS and measure current, then repeat for 124 and 130.  At each steup ensure the light illuminates.

Recorded information: Voltage and current level along with pass/fail illumination.
2.2.2 240VDC source

When this design has been selected this section will be completed.

2.3 Communications

2.4 Environmental Subsystem

Defintion: This subsystem entails the tilt, temperature, pressure humidity, and water sensors.  These tests will be used to confirm proper operation of this subsystem.  This subsystem consist of two components the environmental board and the tilt sensor board.  This section will require these two systems be connected as in the PUP.

Required equipment: The following equipment will be required to run this test:

1) (12V, +5V power supply.

2) Precision level and tilt bench
3) Humidity chamber of 20, 50, and 90% relative humidity

4) Environmetal Chamber 0 to 50(C.

5) Pressure sensor capable of 30 PSIA.

6) Pressure source capable of  1 to 30 PSIA

7) Voltmeter

Setup: Connect +12V to pin 14, -12V to pin 13, +5 to pin 15 and, ground to pin 16.  Mount tiltometer to the tilt bench in the X axis. Assemble Tilt meter and environmental board in Environmental chamber.

Procedure: Set Chamber for 25(C and allow to stabalize.  Measure tilt output voltage for –45, - 22.5, 0, 22.5, and 45.  Then rotate and do the same for the y axis.  Measure output voltage of temperature. Repeat this test with system in environmental chamber at 0 and 50(C.

Disconnect tiltometer for remainder of test.  Place system in thermal chamber in a humidity controlled environment of 20, 50 , and 90% relative humidity.  The themal chamber should be set for 0 25 and 50(C.  Take humidty measurements at each of these point.  

Remove from humidity chamber and attach pressure source to pressure sensor.   While temperature is controlled at 0, 25 and 50(C.  Take pressure measurements at 1, 2, 5, 10, 20, 30PSIA (1%.  

Recorded information:  Record the each output voltage at every data point combination.

2.5 Octal Power Switch Board

Definition: The purpose of these tests will be to determine the functionality of the octal relay boards.  This test will use software on a PC to control each of the relays to confirm operation.

Required Equipment:  The following equipment will be required for this test:

1) Ohm meter

2) 12V power supply

3) Pc software

4) DB25S to DB25P all pins connected straight.

Setup: Conncet the power supply to terminals of X10 with +12V on pin 1 and ground on pin 2 of relay board.  Connect DB cable from PC to relay board. 

Procedure:  Run PC software and turn 12V power supply on.  Measure that all relays Common to Normally closed contact are shorted.  Using software one at a time energize each relay and measure that each individual relay switches to the Normally open state.  Verify that each relays LED illuminates.  Repeat test with power supply set to 10.8 and 13.2V.

Recorded information: Pass/fail of each relay switching and making contact and LED illuminating.
2.6 Power Switch Board

Definition: The purpose of these tests will be to determine the functionality of the relay board. 

Required Equipment:  The following equipment will be required for this test:

1) Ohm meter

2) 10.8 to 13.2V power supply

3)  0 to 5V power supply

4) Environmental Chamber 0 to 50(C

Setup: Connect the power supply to the +12V and Ground terminals  on relay board.  Connect the 5V power supply to the active high input and the ground terminal.

Procedure:  Set the 5V supply for 0V and the 12 to 10.8V. Turn on both power supplies.  Measure that both relays Common to Normally closed contacts are shorted.  Slowly increase power supply until both relays activate.  Record this voltage.  Decrease 5V until both relays de-energize.  Record this voltage.  Repeat this test in chamber at 0 and 50(C.

Recorded information: Pass/fail of each relay switching and making contact and LED illuminating.
2.7 Video Server

Definition: The purpose of this test is to confirm operation of the video server.  This test will be done, by connecting a video source, such as the PUP camera, to each input and, verifying that an image is seen.

Required Equipment:  The following equipment will be required for this test:

1) 20 to 28V variable power supply

2) Video Source (camera is acceptable with NTSC)

3) Computer with 10baseT connection, and web browser

4) Video server manual

5) Environmental chamber 0 to 50(C

Setup: Connect directly from Video server to computer with a null modem or hub  with cat 5 network cable.  Connect power supply to server.  Plug in NTSC source to channel 1.

Procedure: 

1) While applying power (24V) press and hold the Reset switch on video server.

2) Wait for about 5 minutes will server resets

3) Follow direction in manual for first time connection

4) Once the video source can be seen check each of the other three channels for function.

5) Repeat 4 with temperatures of 0 and 50(C and power supply at 20 and 28 volts.

Recorded information:  Record Pass/fail for each channel and configuration.

2.8 Motion Controller Subsystem

Definition:  The purpose of this test is to check the functionallity of the motion subsystem.  The test will be done by connecting up the subsystem a

2.8.1.1 24

2.9 Lkjlkj

