Science Payload Pre- and Post-dive Checklists

Pre-dive

___x__ Remove OBS cap

___x__ Configure IPS software (see Rich Henthorn)

___x__ Check devices.cfg file for appropriate drivers


Run driver test programs for sci payload

___x__
Seabird boardset 1


seabirdTest –dev tcp:arm2:14001

___x__
Seabird boardset 2


seabirdTest –dev tcp:arm2:14002

___x__
ISUS (nitrate)


isusTestSA –off –dev tcp:arm3:14001

___x__
IPS (Ice profiling sonar)

ips4TestSA –dev tcp:arm3:14002

__NA_
Tritech (upward looking sonar)
pa200LR –dev tcp:arm3:14002

___x__
PSA916 (forward looking sonar)
psa916Test –dev tcp:arm4:14002

___x__ Run lamp test on ISUS (see Rich Henthorn)

Post-dive

__x___ Visually inspect internals of science section checking for damage, abnormalities

__x___ Pump clean water through sensors

__x___ Replace OBS cap

Notes

Once again, the SBE temp sensors were pushed back away from the nose, perhaps due to a collision with ice on the surface. Both vertical tube connections were disconnected. Farley and Rich (mostly Farley) took the SBE mounts apart and refit the pieces.

