Science Payload Pre- and Post-dive Checklists

Pre-dive

___x__ Remove OBS cap

___x__ Configure IPS software (see Rich Henthorn)

___x__ Check devices.cfg file for appropriate drivers


Run driver test programs for sci payload

___x__
Seabird boardset 1


seabirdTest –dev tcp:arm2:14001

___x__
Seabird boardset 2


seabirdTest –dev tcp:arm2:14002

___x__
ISUS (nitrate)


isusTestSA –off –dev tcp:arm3:14001

___x__
IPS (Ice profiling sonar)

ips4TestSA –dev tcp:arm3:14002

_____
Tritech (upward looking sonar)
pa200LR –dev tcp:arm3:14002

___x__
PSA916 (forward looking sonar)
psa916Test –dev tcp:arm4:14002

___na_ Run lamp test on ISUS (see Rich Henthorn)

Post-dive

___x__ Observe science section for damage and/or debris (closed fairing)

___x__ Pump clean water through sensors

___x__ Replace OBS cap

Notes: Observed a good quantity of ice clogged in the exhaust of CTD#2 (reflected in dataset as well). Intake tubes appear to be connected.

