Science Payload Pre- and Post-dive Checklists

Pre-dive

__x__ Remove OBS cap

__x__ Configure IPS software (see Rich Henthorn)

__x__ Check devices.cfg file for appropriate drivers


Run driver test programs for sci payload

__x__
Seabird boardset 1


seabirdTest –dev tcp:arm2:14001

__x__
Seabird boardset 2


seabirdTest –dev tcp:arm2:14002

__x__
ISUS (nitrate)



isusTestSA –off –dev tcp:arm3:14001

__x__
IPS (Ice profiling sonar)

ips4TestSA –dev tcp:arm3:14002

__na_
Tritech (upward looking sonar)
pa200LR –dev tcp:arm3:14002

__na_
PSA916 (forward looking sonar)
psa916Test –dev tcp:arm4:14002

___x_ Run lamp test on ISUS (see Rich Henthorn)

Post-dive

__x__ Visually inspect science payload section (note whether fairing on or off).

__x__ Pump clean water through sensors

__x__ Replace OBS cap

Notes:

No damage evident on outside of fairing. All tubing seems to be connected.

