Mesobot LRAUV Configurations 
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a. Load Control
i. C7			3.3V/5V future expansion
ii. C6	xx-232-12	Seabird GPCTD, Serial #, pump 
iii. C5	xx-232-5	Sparton AHRS-M2 Compass, Serial #
iv. C4	xx-232-5	GPS?
v. C3	xx-232-12	C-Star Transmissometer (?)
vi. C2	xx-232-12	WET Labs Eco Triplet, Serial # 
vii. C1	xx-232-12	Aandera O2, Serial #  
viii. C0	 xx---A/D	PAR Licor UWQ #
ix. B7	xx-232-12	Iridium ?, SN, IMEI: 
x. B6	 xx-off-12	Cradlepoint WiFi/3G, Serial #, IMEI 
a. IP wired: xxx
b. IP cell: xxx
xi. B5 XXXXXXX	3/5/12 Power Converter			
xii. B4    xx-232-24-5A DVL/ADCP, Serial #  
xiii. B3    xx-232-24-5A	Benthos DAT or Micromodem Acoustic Modem, Serial #Tx  
xiv. B2    xx-232-Batt-5A Lights
xv. B1	xx-232-12-5A	Camera housing (cameras, TX2,..?)
xvi. B0	xx---A/D	Depth sensor Keller PA-6ST, SN XX
xvii. [bookmark: _GoBack]A7	xx-232-Batt-5ASUPR?
xviii. A6  	xx-232-Batt-5A Release motors (?)
xix. A5 	xx-485-Batt-5A Thruster channel 1
xx. A4	xx-485-Batt- 5A Thruster channel 2
xxi. A3	xx-485-Batt-5A Thruster channel 3
xxii. A2   	xx-485-Batt- 5A Thruster channel 4
xxiii. A1   	xx-485-Batt-5A 5A EzServo Variable ballast pump (5A)
xxiv. A0   			Spare Analog Expansion
2. Standalone relocations
a. Benthos transponder 26/29 kHz , Serial xxxx, 26/29 kHz 
b. Telonics Argos/VHF beacon #xxA,160.785 MHz, Standalone battery powered
3. Notes:  
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