Mesobot Load Control Configuration 			9/5/17 
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a. Load Control
i. C7	xx-232-12		Stereo Cameras			3.3V/5V future expansion
ii. C6	xx-232-12		Science Camera 
iii. Seabird GPCTD+O2 Serial #, #, # 
iv. C5	xx-232-5		Sparton AHRS-M2 Compass, Serial #
v. C4	xx-232-12		Satlantic PAR		
vi. 
vii. 
viii. xx-232-5		GPS?
ix. C3	xx-232-12		Seabird GPCTD+O2 Serial #, #, # 
x. xx-232-12		C-Star Transmissometer (?)
xi. C2	xx-232-12		WET Labs Eco Triplet, Serial # (could share with CTD)
xii. C1	xx-232-12		GPS/Iridium Xeos Apollo, Serial #, IMEI: 
xiii. xx-232-12		Future expansion
xiv. C0	 xx-232-12---A/D		DSL modem, tether dropperPAR Licor UWQ # (?)
xv. B7	xx-232-12		Iridium ?, Serial #, IMEI: XXXXXXX		3/5/12 Power Converter
xvi. 
xvii. [bookmark: _GoBack]B6	XXXXXXXX		24 VDC Power converter
xviii.  xx-off-12		Cradlepoint WiFi/3G, Serial #, IMEI 
xix. IP wired: xxx
xx. IP cell: xxx
xxi. B5 XXXXXXX		3/5/12 Power Converter	xx-xx-12		TX2, ethernet switch, video recorder & encoders
xxii. 		
xxiii. B4   	xx-232-Batt-5A 	SUPR microbial sampler with large pump
xxiv.  xx-232-24-5A 		DVL/ADCP, Serial #  
xxv. B3	    xx-232-24-5A		Benthos Acoustic Modem, Serial #  xx-232-24-5A		Benthos DAT or Micromodem Acoustic Modem, Serial #  
xxvi. B2  	  xx-232-Batt-5A 	Light 1 – MultiRay – dimmed to 50% 
xxvii. B1	xx-232-Batt-5A 	Light 2 - MultiRay – dimmed to 50%
xxviii. 
xxix. xx-232-12-5A		Camera housing (cameras, TX2,..?)
xxx. B0	xx---A/D			Depth sensor Keller PA-6ST, SN XX
xxxi. A7	xx-232-Batt		Release Motor
xxxii. A6	xx-485-Batt-5A 	Variable ballast pump (5A)
xxxiii. A5 	xx-485-Batt-5A 	Thruster channel 1
xxxiv. A4 	xx-485-Batt-5A 	Thruster channel 2
xxxv. A3	xx-485-Batt- 5A 	Thruster channel 3
xxxvi. A2	xx-485-Batt-5A 	Thruster channel 4
xxxvii. A1   	xx-485-Batt- 5A 	Thruster channel 5
xxxviii. A0   	xx-485-Batt- 5A 	Thruster channel 6xx-232-Batt-5A 	SUPR?
xxxix. A6  	xx-232-Batt-5A 	Release motors (?)
xl. A5 	xx-485-Batt-5A 	Thruster channel 1
xli. A4	xx-485-Batt- 5A 	Thruster channel 2
xlii. A3	xx-485-Batt-5A 	Thruster channel 3
xliii. A2   	xx-485-Batt- 5A 	Thruster channel 4
xliv. A1   	xx-485-Batt-5A  	Variable ballast pump (5A)
xlv. A0   			
Spare Analog Expansion
2. Standalone relocations devices
a. Benthos transponder 26/29 kHz , Serial xxxx, 26/29 kHz 
b. Telonics Argos/VHF beacon TAM-4310-3,160.785 MHz, Standalone battery powered
3. Notes:  : *** Light output limited to 50% to keep under ~60 watt
 limit of load control board and backplane with all thrusters running.  We may still exceed the limits of the backplane so we need to define the worst cxase system maximum current.***
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