Goals: jelly tracking algorithm that tests cameras + lighting configuration on August 29/September 1st: (1) test three lighting modes: single, same-axis; double, same-axis; single, off-axis; double, off-axis; change separation between lights, (2) use wide-angle cameras to increase working FOV?

Mike on vacation July 17th-28th 

Meeting action items:

Brian: send off documentation describing LRAUV (completed)
Brian: confirm 10hz control at the motors via a load test on the existing LRAUV bench system using the backseat driver interface
[bookmark: _GoBack]Brett: follow up with Ed to check on electrical drawings hand-off to WHOI
Kakani: resolve Mesobot internal proposal issue
Brett: follow up about pricing of cameras 
Steve: ask Godwin about setting up Matlab for SUNET ID holders
Brett: find lights (4?) and 80/20 for lightmount
Kakani: talk to Mark Chaffey about lighting configuration on I2MAP, do we need light from both sides
Kakani: talk to Dale about wide-angle camera

Needs from WHOI:
1. What’s the nominal vehicle configuration? Need to know before testing. Need opportunity to comment.
2. What’s the nominal camera/lighting configuration? MBARI wants two wide-angle, monochrome cameras for stereo
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