[bookmark: _GoBack]Goals: jelly tracking algorithm that tests cameras + lighting configuration on August 29th to test three lighting modes: single, same-axis; double, same-axis; single, off-axis; double, off-axis; change separation between lights

Mike on vacation July 17th-27th 

Meeting action items:

Brian: confirm 10Hz control at the motors via a load test on the existing LRAUV bench system using the backseat driver interface (in progress)
Brett: follow up with Ed to check on electrical drawings hand-off to WHOI (in progress)
Kakani: work on progress reports, due mid-August (completed)
Kakani: email Kandace with brief description of postdoc project (in progress)
Kakani: ask Steve about bioluminescence of larvaceans, illumination, etc. (in progress)
Steve: speak with Stanford CS faculty about postdoc opportunities and larvacean processing student projects (in progress)
Mike: using ROV video, track using downsampled video to determine resolution thresholds (in progress)
Kakani: talk to Francisco about accessing current profile data near M1 for Mesobot mission planning and share with Dana for buoy/tether testing (completed)
Kakani: talk to Denis about sharing rolling shutter timing data with Mesobot group (in progress)
Kakani: email Dale and ask if he could bring back his DSPL HD-wide angle
Brett: get quotes on camera/light hardware


Needs from WHOI:
1. What’s the nominal vehicle configuration? Need to know before testing. Need opportunity to comment.
1. What’s the nominal camera/lighting configuration? MBARI wants two wide-angle, monochrome cameras for stereo
1. How are they importing video to TX2? Connecting USB camera directly to board.


oy g s s g crton o gt
e S

M oncain oy 7270
[re—

o —
b b Ty
SR
T,

o e
B

e
LT M ——
e

o o
ol T e L)
e

ST e sttt g ienge
e

-
e o ot MO vt i




