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THIS DOCUMENT IS ISSUED IN STRICT CONFIDENCE


ON CONDITION THAT IT IS NOT COPIED REPRINTED 


OR DISCLOSED TO A THIRD PARTY EITHER WHOLLY 


OR IN PART WITHOUT THE PRIOR WRITTEN CONSENT
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DRAIN WIRE-1 UNIT


Awg No. 26(19 x 0.004”) B/C





TAPE


Aluminum Mylar Tape





TAPE


Mylar Tape





INNER JACKET


Polyethylene 


Color: Black





ARMOR-STEEL WIRES


Two Layers of Spaced GIPS





OUTER JACKET


Polyethylene


Color: Orange


























Nominal O.D.----------------------


Weight in Air----------------------


Weight in Seawater---------------


Breaking Strength-----------------


Maximum Load-------------------


Min. Bend Diameter--------------








ESTIMATED VALUES





TWISTED PAIRS-2 UNITS


Awg No. 26(7 x 0.0063”) B/C


DC Resistance @ 20° C ≤  46.0 Ohms/1000 Ft


Polypropylene Insulation


Voltage Rating: 600 VDC


Two Conductors Twisted


Color Code: Black-White & Red-Blue


Polyethylene Belt (natural color)


Nominal  Impedance: 100-120 Ohms








INTERSTICES WATERBLOCKED








INTERSTICES WATERBLOCKED








SINGLE CONDUCTORS-12 UNITS


Awg No. 26(7 x 0.0063”) B/C


DC Resistance @ 20° C ≤  44.5 Ohms/1000 Ft


Polypropylene Insulation


Voltage Rating: 600 VDC


Color Code: Brown       Yellow    Violet       White


                     Red           Green      Gray         Tan


                     Orange      Blue        Black        Pink














0.480”


140 Lb/1,000 Feet


55 Lb/1,000 Feet


3,200 Pounds


800 Pounds


16 Inches








