FNMOC High Resolution SST/Sea Ice Analysis for GHRSST

These fields are a contribution to the GODAE HiRes SST pilot project.

The analysis is updated every 6 hours using AVHRR GAC satellite SST and in

situ SST from ships and buoys (fixed and drifting). Sea ice concentration

observations are from the SSM/I instrument on DMSP. All sea ice and SST

observations are quality controlled prior to being used in the analysis. The

grid lat/lons are contained in two files (grdlat, grdlon). The grid is a near

global mercator projection with dimensions of 3241 x 2441 (12 km resolution at

the equator, ~9 km resolution at mid-latitudes). The files are 32 bit direct

access files with record lengths of 31,645,124 bytes.

Ascii format grid definitions may be found in the GrADS .ctl files.

Binary grid definitions (also 32 bid direct access) are in:

grdlat_sfc_000000_000000_1o3241x2441_00000000_datafld

grdlon_sfc_000000_000000_1o3241x2441_00000000_datafld

http://www.usgodae.org/ftp/outgoing/fnmoc/models/ghrsst/docs/
