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This document outlines the trade-off study to be performed at MBARI to promote an understanding of the design-space relevant to the station keeping buoys envisioned by DARPA for long-term hydrophone support.  The current solutions being pursued by the participants of this program were tested during the technology demonstrations held at MBARI in October 2007.  A wide range of approaches pursued by the current program participants indicates that the current understanding of the problems and options for developing these systems is not sufficiently understood.  

The goal of this study is to analyze the design space sufficiently to determine which trade-offs are significant design drivers and identify any optimizations that should be considered.  The aim is to give the system designers a basis for aiming future development in a direction that has the highest probability of generating an optimized solution to this difficult engineering problem. 
Trade-Study Overview

There are three classes of variables that need to be considered in a design-space investigation; 
a. The environmental conditions at the target deployment locations.  (wind speed, wave height, and solar insolation.)

b. Those that affect the performance of the system in given environmental conditions.  These variables include those related to what energy sources are utilized, how that energy is collected and stored, and how that energy is applied to keep the buoy on station and performing the needed tasks.  
c. Design variables that affect the operational utility of the system. (size, weight, reliability, and cost).
Although there is significant interplay between these three classes, it is useful to consider each individually to minimize competition between the factors that drive the final choices to promote an understanding of the underlying performance issues.  For instance, an analysis of the performance factors may drive the design towards a size and weight scale that can not be accommodated, but at least design choices will be made with a clear understanding of the trade-off being made (performance versus size).  Similarly, the environmental conditions the system shall operate in will vary from site to site and an understanding of the capabilities of different techniques will aid in designing systems that will be successful across a range of sites.
The goal of the study presented below is to identify which part of the design space should be concentrated on to meet the requirements and to identify optimal design choices related to system performance in a variety of conditions.  Coupled with an analysis of environmental conditions at a range of likely deployment sites, it is expected that some optimal design choices will be evident.  
Finally, data collected during the October 2007 demonstrations in Monterey Bay may be useful in the context of the design study results, providing a comparison basis for the performance factor analysis.
Trade-Study Outline
To achieve this goal, a number of specific tasks will be undertaken as follows: 
Analysis of design space

1. Analysis of environmental conditions at projected sites.

a. Expected energy fluxes in sun, wind, and waves.

b. Expected currents

c. Relative directions of currents, wind and waves

d. Expected temporal variability of above

2. Analysis of potential energy of various energy sources (solar, wind, wave)

a. Analysis of possible conversion efficiencies of various sources.

b. Analysis of energy storage efficiencies.

c. Analysis of platform energy requirements

i. Station keeping (depends on environmental conditions)

ii. Sonar tasks (may depend on station keeping accuracy?)

iii. Communications

3. Review of operational constraints and form-factor goals.
Design trade-off evaluation
1. Identification of important variables in the design space.

2. Analysis of potential optimization within the range of design space variables.

3. Analysis of sensitivity of trade-offs to deployment site conditions. 

4. Effects on trade-space due to limitations imposed by operational/form-factor constraints
Analysis of 2007 demonstration data 
1. Analysis of energy harvesting efficiency.
2. Analysis of energy use efficiency.

Example:  Station Keep against a Current with Wind Energy in Monterey Bay
For this example we use wind and current data, acquired in Monterey Bay from MBARI’s M1 mooring since 1992.  The record is not continuous for all sensors, and we limit the study to the portion of the data set in which both the current and wind data is good.  The resulting data set has 84903 hourly observations.  Figure 1 shows an extract of the data set.
We can compute wind power per unit area by the following formula:

[image: image1.wmf]3

1

2

windo

Pv

r

=


For the purposes of the calculations below we approximate the density (a) of air as 1.168 kg/m3, ignoring the effects of changing atmospheric temperature, pressure and humidity.  The power associated with the prevailing ocean currents is also important, and is calculated using the same formula, using a seawater density (o) of 1025 kg/ m3, ignoring variations in salinity and temperature.  Figure 2 shows the probability that the current power is below a given level.  Thus 90% of the time the current has a power less than 7 W/m2.  Figure 3 provides an equivalent plot for wind power, showing that 90% of the time the wind power is less that 435 W/m2.  
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Figure 1:  An extract of the M1 data set, showing wind and current speed at 20 m depth, and wind and current direction for a four day period.
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Figure 2:  Statistics of current power.  This plot shows the fraction of time the current at 20 m depth is less than a given power level.  
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Figure 3:  Statistics of wind power.  This plot shows the fraction of time the wind is less than a given power level.  
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Figure 4:  Log probability distribution as a function of both current and wind power.  Note that periods of high current power occur most often when winds are low and visa versa.
Note that the current used for the 

Example Station-Keeping Buoy Model
For this example, we consider a buoy which generates power using a wind turbine, and maintains station with a water propulsion system.  We simplify the problem using the following assumptions:

1) Drag in the water is dominated by a hydrophone cable with total area (Ad) of 0.47m2 (assuming a diameter of 3/8” and a length of 50m) and drag coefficient (Cd) of 1.0.  
2) Propulsion in the water is provided with an efficiency (p) of 0.5 (electrical through delivered thrust) by a propulsion system acting over an area Ap of 0.2 m2.  Energy is provided by a wind turbine with efficiency (g) of 26% and area Ag,  of 1.0 m2 where efficiency is defined as conversion of wind power to electrical power.
The forces acting on the buoy are thus the current drag of the cable, the reaction force on the wind turbine, and the force exerted by the propulsion system to keep the buoy on station.  The drag force is:
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The reaction force for the wind generator is found by solving for the exit velocity of air from the wind turbine, vout and using the change in air velocity to compute the force.  
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where 
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 are the unit vectors in the direction of current and wind, respectively.  The solution for vout is not given here as it is lengthy and does not add materially to the discussion.  
To maintain station, the propulsion unit must impart a change in velocity to the water (v).  Assuming the change in velocity is much greater than the perturbing currents, the power required is related to the drag and reaction forces by:
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Using the parameters defined above, and the environmental data from M1, we compute the power needed for station keeping, and the power generated for a period when the currents are unusually high.  This is shown in figure 5.  Figure 6 shows the 
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