Duration of the rods seals for each iteration:
Engineer: François Cazenave
Date: 1/14/19

First iteration:
55 days of operation. Seal did not fail.

Second iteration (harder seals):
61 days, Seals did not fail.

Second iteration, seals replaced:
132 days, with compliant plate. Seal failed, gas leaked into the hydraulic chamber. (seals may have started failing earlier than 132 days)
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Third iteration (opposing double seals with check valve)
31 days with compliant plate, 7 days with flapping foil (minimal stroking), 54 days with heave cone.
Total 92 days.
Seals failed, gas leaked out of check valve.

Conclusion:
