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Cable type:
5/16” nilspin mooring wire. We usually use old wire from the MBARI moorings, after careful inspection.

Cable length is 120m. This is for a deployment in 80m water, and with the submerged plate hanging at 30m depth. A 40m chain is also used. So the total length is 30 + 150 + 40 = 220m. 
Terminations:
Crosby 5/16” swage sockets (crosby  S502) are used on each end. Filler wire are used inside the socket.
Carpenter rigging in SF has put on the terminations for us several time.
Silicon is applied inside the socket and the strain relief boots.
Strain relief boots are used. The strain relief boots have been bored out to 57/64” to fit the swage sockets,
