10020546_1 README_FAB.TXT

Design Contact: John Zsori, CID+ - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
Cell:    408.391.6656
email:   john_zsori@pacbell.net

REFER ALL PCB DESIGN RELATED ISSUES TO JOHN ZSORI

Client: MBARI
7700 Sandholdt Road
Moss Landing, CA  95039
Wayne Radochonski - 831.775.1700


Fabrication data included in 10020546_1-CAM.ZIP:

                PowerPCB Gerber Files (RS-274-X Format)
      
10020546_1-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Primary (Top) Side)
10020546_1-ST.PHO     Primary Silkscreen (Top)
10020546_1-SB.PHO     Secondary Silkscreen (Bottom)  
10020546_1-MT.PHO     Primary Solder Mask (Top)
10020546_1-MB.PHO     Secondary Solder Mask (Bottom)
10020546_1-PT.PHO      Primary Paste Mask (Top)
10020546_1-PB.PHO    Secondary Paste Mask (Bottom)
10020546_1-DD.PHO     Drill Drawing
10020546_1-DD.PDF     Drill Drawing in Adobe format

	Drill Files

10020546_1-NC.DRL     NC Drill

                Netlist

10020546_1-IPC.NET    IPC-D-356 Format Netlist (See Note 2)

Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask 
size to your specific manufacturing tolerances while maintaining maximum web.
Fine pitch devices may be gang masked as necessary.

2. Compare the IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.
