EyeRIS Dive Operations

Pre Dive
1. Check hardware visually
a. Clean camera and light ports with wipes
b. Check for loose fittings
2. Power on ROV and check Camera Ethernet comms (internal sensors, etc)
3. Plug all four coax connectors into PHT4 FG box and confirm it as power.
4. Turn on camera power and confirm PHT4 FG box shows no flashing lights
a. Flashing red means no light on that channel
b. Flashing green means weak signal and data recoding is not possible
5. Open up RxLive and wait for the “Updating” message in the bottom right corner to change to showing GPU memory
6. Once the GUI has updated, click on camera on open
7. Confirm camera is working as expected
8. Click on Export and select sequence output, set file path and file prefix as desired
9. Turn on light power and confirm all lights are working up to 100%. Turn off lights until vehicle is in the water

Dive
· For MiniROV, Turn on O2 sensor
· Turn on lights at 100% and check GUI shows 100% output
· Check exposure time, fps and set sequence recording for mission
· Periodically check the following during dive:
· Lights at 100% output
· Available disk space on E: (Storage)
· Camera settings

Post Dive (During Recovery)
1. Turn off lights before the vehicle leaves the water
2. Start copying data from Storage to external USB drives
3. Close RxLive and turn off power to camera
4. [bookmark: _GoBack]Unplug 4 coax connectors from PHT4 FG module.

