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Sensor:  NOIP1SN025KA-GDI (ON Semiconductor)
Sensor type:
CMOS
Resolution: 5120x5120 px
Pixel Size:  4.5µm
Sensor Size:  23.04x23.04mm
Shutter type:  global shutter
Max. frame rate:
80fps

Interface type: CXP-6 4 Lanes (up to 6.25 Gbit/s per lane)
Power over CoaXPress:
yes
Connectors on camera:
4 x female
 
Lens mount  M58x0.75 or F-mount
Size (w / h / d) 70x71x51mm (F-mount adapter adds 35mm)
Weight 300 g
Ambient temperature -10 bis 45 °C
Protection class IP40
 
Power consumption
13W
 
Trigger intern / extern / software
Trigger edge high / low 
Trigger IN TTL-24 V 
2
Outputs open drain 
4
Optical in  1
RS-232  1 x in / 1 x out
 
IO connector  Hirose 12pin (HR10A-10R-12P)
Mating connector
HR10A-10R-12S
 
Frame grabber:
Euresys Coaxlink Quad (I will send you the link to the model we use)


