BatterySpace.com Customized Battery Pack Inquiry Form
Dear Customer, 

Thanks for contacting BatterySpace.com.  Here are few things to know before start.

1. There will be a one time prototype fee for each kind of custom battery pack. Depending on how complicated  the battery’s configuration, the minimum will be $80 for Nimh & Nicd Battery Packs,  and $150 for Lithium battery packs. 
2. Due to the shipping regulation from the Department of Transportation (DOT) for lithium batteries, battery packs must pass UN38.3 before ship by air. So prototypes of Lithium batteries must be shipped by Ground, class 9 package, and UPS/Fedex will charge an extra handling fee per box handling fee on top of regular shipping cost.  
For shipping addresses outside of the USA, sorry we can’t ship Lithium battery prototypes to you.  Suggest to choose battery packs with UN38.3 from the following links. 
Lithium Ion:  http://www.batteryspace.com/li-ion-battery-packs-with-un-38-3.aspx
LiFePO4: http://www.batteryspace.com/UN-Approved-LiFePO4-Cells-/-Packs.aspx
3. If the production of Lithium battery packs is over 100pcs/annually, it is required to get the battery UN 38.3 Tested before allowing it to be shipped. This is an extra cost in addition to the cost of a custom battery pack that you must be responsible for.  We can help you to get your pack UN38.3 tested or you can do it yourself from other testing labs. For more detail, please check our UN38.3 Safety Test page. 
	Your name: Paul Roberts
	Company Name:  MBARI

	Telephone: 831-774-1842
	E-mail: proberts@mbari.org

	Please fill the information as much as you can, which will help us to choose the correct components. If unknown, please leave it in blank

	Battery Type:
Li-Ion, LiFePO4, NiMH, NiCd, or Polymer
	Li-Ion
	Cell size 
(If NiMH, enter AA, C, D, Sub C, F etc.)
If Li-Ion, enter battery size (14500, 18650…)
	18650 in 2P4S

	Battery Pack Voltage (V)
	14.8 nom
	Battery Pack Capacity (AH)
	~ 80 Whr

	Max. Discharging current (A)


	30 A
	Estimated Wattage in your DC Device
	50W

	Continuous Discharging Current (A)
	20A at 20% duty
	Expected running time for your device
	NA (on external power)

	Max. Pulse Current (A) 
	30A
	Battery Size requirement (Inch) ( LxWxH)
	6.6 x 2.7 x 1.1

	Duration of Pulse Current (ms)
	10
	Wire Length (Inch)
	10”

	Connector type
	Bare Leads
	Wire Gauge (AWG)
	16 AGW

	Applications
	Charge capacitor bank for video strobe circuit

	Other special requirements
	

	How many packs do you need?
	10


Battery Configuration

If the customized pack is made by cylinder Cell,   Please use the following green round circles to make drawing.  If you need more circles, please click and drag one from right corner. 


If the customized pack is made by prismatic cell ( Polymer Li-Ion ),  Please use the following gray rectangular to make drawing.  If you need more rectangular, please click and drag one from right corner.




You can also make simple hand drawings by any methods and email us. 
BatterySpace.com 825 S. 19th St., Richmond, CA, 94804

                             Phone# 510-525-2328, Fax; 510-439-2808 email: sales@batteryspace.com       Date: 7/18/2022

