TRANSMIT BLOCK

The transmit block is responsbile for routing data from one line out all the other lines. The NAND gate accepts signals from the other three sections, and routes them out the seciont output port. (The +5 gate is unused and tied high).
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