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Abstract - New inovative scientific underwater cable networks have been proposed and initiated all over the world. Although these network become feasible due to recent evolution in underwater telecommunication cable technology, their Communication systems are quite different from the telecommunication cable systems. 

In this paper, difference between those systems and basic technical requirements against scientific underwater cable network will be firstly described. There are some options to realize communication systems. These options,including optical GbE over DWDM, CWDM and DWDM with Raman modulators, will presented with their advantages and disadvantages.  The present status of NEPTUNE communication system  and consideration on reliability will also bepresented.

I. INTRODUCTION

Recent progress in optical telecommunication underwater cables and other related technologies make it possible to develop versatile, next generation scientific cables. These networks will provide electric power and wide range of data transmission capabilities to many kinds of equipment deployed on seafloor. They enable researchers to access seafloor equipment in real-time from laboratories and provide long-term, real-time data from the seafloor. They are expected to bring breakthroughs to multidisciplinary science fields.

In fact, new scientific underwater cable network projects are being proposed all over the world.. In USA and Canada, NEPTUNE, MARS and VENUS projects have been proposed and initiated. NEPTUNE, a joint project between the USA and Canada, will realize a vast cable network of 3,000km in total length in the north-west Pacific. MARS in Monterey Bay and VENUS in Canada precede NEPTUNE and are regarded as test beds for NEPTUNE. In Japan ARENA project has been proposed by IEEE OES Japan chapter. It will construct a scientific underwater cable network covering both sides of plate boundaries. ESONET project in EUROPE will cover from Mediterranean to north Atlantic Ocean

Communication systems being proposed for these scientific cable networks are significantly different from optical underwater telecommunication cable systems and communication systems built for the telecommunications industry. Most communication terminals (and associated optical transmitters and receivers) for these scientific observatories are placed in underwater housings that are not easily accessible for regular maintenance or repair. Conventional underwater telecommunication cable systems connect only to stations (communications terminals) on land.


It is not affordable for the oceanographic research community to fund new research, development, and product qualification for telecom submarine-grade optical network equipment. It is reasonable for the oceanographic research community to determine if existing or soon-to-be-existing commercial off the shelf (COTS) optical network products can be made to work adequately in the submarine environment.

From a conceptual design standpoint, designs of terrestrial and undersea optical networks can be seen as almost identical. However, from a practical standpoint, submarine optical networks require equipment with low electrical power requirements, small physical size, sufficient heat dissipation and heat tolerance, high reliability, and no need for physical access by a technician. Thankfully, the demands of the terrestrial optical networking marketplace are driving products in these directions. Our ocean observatory design efforts continue to benefit by piggy-backing on these ongoing R&D efforts.

One disadvantage to the rapid advances in optical network product development is that the rapid emergence of new and attractive types of optical network equipment  can sometimes interrupt current design efforts because of their potential cost and design benefits. Thus, it is important to know the projected deployment date for an observatory so that one can work back to a design freeze date for the optical network. Given the typically fixed-cost nature of the observatory development efforts described here, the cost ramifications of freezing the design too soon can have significant affect on the geographic scope and features of the resulting observatory.

The remainder of this paper presents a snapshot of the optical network alternatives currently being considered by the NEPTUNE and ARENA ocean observatory data communications design teams. In the next section we examine the requirements for each of the design efforts. Section III sketches the technical aspects of the alternatives available for optical network transport equipment. In section IV we review how node and network reliability can be accomplished using commercial-off-the-shelf equipment.  Finally, in section V we review the status of the NEPTUNE and ARENA efforts and identify the current set of design decisions pertaining to each.   

II. BASIC CONSIDERATIONS AND REQUIREMENTS


It is important the choices made for the optical network design be based on the individual requirements for each of the observatories. Major considerations and requirements are listed below. 

A.
Network Configuration


All transoceanic commercial telecommunications systems are point-to-point links connecting terrestrially shore to shore, with only a few occasional branches. On the other hand, in the case of a scientific cable network, most sensors, instruments and optical transmitters/receivers are placed on the seabed. The cable networks are required to branch in order to economically deploy sensors two-dimensionally in scientifically interesting area. These requirements are thoroughly different from those for telecommunication systems, and make specific characteristics for scientific cable networks.

B.
Flexibility and Expandability


The scientific network often needs to grow with incremental funding, unpredictable scientific needs and future changes in requirements as more sophisticated sensors are developed. Thus the data transmission system should be flexible and expandable to accommodate these changes and expansions.

C. Signal Hierarchy and IP Network.

Conventional underwater and terrestrial telecommunication systems operate with SONET systems. Although they provide reliable and wide band data network, they lack flexibility and expandability. They are for point-to-point connect systems. Moreover, SONET systems are for public telecommunication systems to which a high reliability is required, and are not commercial off-the-shelf (COTS) systems.


One promising system is an IP-based network. The IP network allows for topologically independent extension and enlargement without affecting other nodes. The present scientific community as a majority operates over IP an network which is manageable with commercially available data processing techniques prevalent in the Internet sphere

D.
Reliability and Cost

The reliability requirement for scientific cable networks is shared with commercial telecommunications. As most of transmission terminals will be placed on seafloor, it is not easy, highly costly and time-consuming to repair or maintain these devices. However telecomm grade reliability is attained through a high cost, which is recouped through a business model that research does not comply with. Further, there is a likelihood of occasional system modification for a research network from time to time, during which repairs and upgrades could be engaged. Therefore the reliability of an underwater research network must conform to a different cost/reliability model when compared with commercial telecommunications.

The underwater repeaters for telecommunication systems consists of only qualified devices and have a simple structure to realize high reliability. On the other hand, the underwater systems for scientific cable networks would contain many devices such as Ethernet switches, sensor interfaces and optical transmitter/receivers. It is not realistic to make these devices from qualified devices only. It is needed to use COTS devices to realize a system which satisfy scientific requirements. This means that further measures to increase reliability is needed.

One fascinating solution would be mesh or ring networks. In mesh or ring networks, even if a portion of the network breaks, the network can continue working bypassing the broken portion. This can also increase the reliability for power feeding systems. By increasing both equipment and path redundancy we can obtain availability of the system without the use of extremely costly high reliability devices. 

Redundancy should be considered for most critical or vulnerable devices.

E.
Transmission Capacity

Transmission capacity requirements can be classified into three categories.

1) HDTV signals

Bandwdith requirements for HDTV depends on the signal compression mode. In the satellite broadcasting system in Japan, the baseband HDTV signal of 1.5Gbps is compressed to 24Mbps with MPEG2 which enables recording on D-VHS recorders for home use. The quality of images depends on the compression rate. Although the degradation of images is very little even if high compression rate of 0.016 (satellite broadcasting system) is used, the acceptable level of degradation for scientific use should be re-considered. In the re-consideration, terrestrial transmission and video recording should be taken into consideration.

In addition, if the HDTV signal is transmitted over Ethernet, dropouts of packets could seriously affect the decompression process and may deterioriate the image quality. Quality of service requirements may be significantly increased for the subsea Internet if this is the case. If full-bandwidth HDTV is required for subsea science it is probable that a dedicate path (packet or wave) may be required.

2) Time Synchronous Signal
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For acoustic geodesy, time synchronous signals with accuracy from 5-10 micro-seconds is needed.

In case of IP, the NTP protocol typically provides an accuracy of time synchronization is typically in order of milliseconds or higher. Another transmission path is likely needed for a time synchronous signal.

3) Other Data and Control Signals


There are many kinds of sensors and instruments connected to scientific cable network. Although the amount and the format of these data and control signal is different from each other, the total amount of data would be far less than that for the HDTV signal. IP networks can provide flexible infrastructures which accommodate these various kinds of signals.

F. Node to Node Communication

With the advent of sensor network technologies [ ], a more recent need has emerged for low-latency node-to-node interactions. If this proves to be a serious need it limits the topologies available for the optical network design.

III. TECHNICAL OPTIONS

There are several technical options available. Optical communication technology is evolving very rapidly, and the most promising options would change in time. However, it is worthwhile to examine the characteristics of the currently available options and describe their advantages and disadvantages, as well as the applications they are suitable for. This will help to make clear the present status and orientations of both the NEPTUNE and ARENA development efforts (which will be further discussed in section III.

1) Optical GbE over DWDM with Intra-node Redundancy

The optical solution for NEPTUNE, which appears to be the most promising at the time of this writing, is a Gigabit Ethernet over DWDM solution. Using commercially available optical transponders, EDFAs and multiplexing equipment distances in excess of 150km are expectable with equipment that works within thermal, electrical and dimensional parameters acceptable for oceanographic deployment. The availability of affordable EDFAs for terrestrial use allows preamplificaction on the order of 23dB.

The NEPTUNE design projected recently uses 8 wavelengths carrying 1 GbE. With an 8 ITU wavelength solution, the commercial equipment is greatly simplified, since the Demux gratings need not be temperature stabilized. DFB lasers in the transponders are stabilized via Peltier coolers.

The NEPTUNE project has presently tested in the laboratory, commercial off-the-shelf (COTS) optical Ethernet devices by Network Electronics, which prove the viability of an optical Ethernet solution for underwater research networks. Distances of 50km un-amplified and over 100km amplified using SMF28 type fibre have proven to operate with BER rates better than 10-12. This equipment operates an appropriate thermal output range and electrical power range compliant with the NEPTUNE power system design.

[image: image4.bmp]
The various characteristics of the system tested in the laboratory are shown in the table below.

	TABLE I

DWDM CHARACTERISTICS

	Typical Transceiver Specs (Network Electronics Transponders)

	Wavelength:
	1528 nm – 1562 nm

	Wavelength Output Power:
	+0 dBm out

	Receiver Sensitivity:
	-19 dBm in

	Dispersion Penalty:

	2dB @ 17km (Nortel Lasers)

	Typical WDM Parameters (Network Electronics Mux/Demux)

	Mux Attenuation:
	4dB

	DeMux Attenuation
	5dB

	Common Telecomm Fiber Specs (Corning SMF28E)

	Attenuation:
	0.19 dB @ 1550 nm

	Dispersion:
	18 ps/(nm.km)

	EDFA Preamplifier Specifications (Nortel/Bookham 1AOC28)

	Gain:
	23 dB

	Maximum Input:
	-10 dBm

	Optical Budget Estimate – 178 kilometer maximum

	Input
	0 dBm

	Attenuation
	3(mux) + 3(demux) + 2(dispersion) + .19dB/km x 178km – 23(gain) = 19dB

	Output
	Input – Attenuation = -19dBm


2) GbE over CWDM Alternative

One approach to optical networking, which has shown promise in recent years, is CWDM technology. This method has assets similar to DWDM however with a greater limitation of distance. The Mux/Demux equipment investigated for this technology is generally of a higher attenuation compared to DWDM. Equipment from Cisco Systems, Inc. has a per wavelength attenuation of 9dB for the Mux/DeMux pair. In addition the fiber attenuation is slightly higher for the broader frequency range of CWDM, being about 0.24 dB/km over SMF28E at 1470nm.

The attenuation problems mentioned are not surmountable using amplification as of this writing. The SOA (semiconductor optical amplifier) devices presently available are relatively new and have not developed a reliability profile comparable to EDFAs. Also the SOA still has some issues with crosstalk and similar effects at 1Gb signal rates. Thus the likely sphere of application for CWDM is for unamplified networks with node separation less than 80km or as extension networks to a network deployed over a large geographic area. There is some reliability, cost and dimensional advantage when the amplifiers are omitted. Cisco Systems, Inc. presently offers a complete solution, which is rather compact. (The Mux/Demux is 21.15 x 43.35 x 26.52 cm)
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The NEPTUNE project has evaluated, at a "spec sheet" level, CWDM equipment for use with NEPUTNE. We have not elected to test it in the laboratory for NEPTUNE. This is due to its apparent attenuation limited functionality at about 70km. However CWDM appears to be very attractive for a small system connecting 1GbE networks at distances of around 50km. Recent enhancements to the 14XXnm peak in Corning fiber of furthered this cause. The facile nature IP/GbE mentioned for the extension of NEPTUNE also plays handily in it's ability to interconnect with other GbE optical protocols. 

A set of characteristics we envision for a possible simple CWDM extension node design for NEPTUNE are shown below.

	TABLE II

CWDM CHARACTERISTICS

	Typical Transceiver Specs (Cisco CWDM GBICS)

	Wavelength:
	1470nm - 1610nm

	Wavelength Output Power:
	+3 dBm out

	Receiver Sensitivity:
	-29 dBm in

	Dispersion Penalty:

	3dB

	Typical WDM Parameters (Cisco)

	Mux Attenuation:
	4dB

	DeMux Attenuation
	5dB

	Common Telecomm Fiber Specs (Corning SMF28E)

	Attenuation:
	0.24 dB @1470nm

	Dispersion
	18 ps/(nm.km)

	Optical Budget Estimate – 80 km. maximum

	Input
	0.24 dB @1470nm

	Attenuation
	4(mux) + 5(demux) + 3(dispersion) + .24dB/km x 80km = 31dB

	Output
	Input – Attenuation = -29dBm


[image: image6.jpg]o o o
'S o 3

10 Year Success Rate of 6 Node String

o
N

Node Reliability at 10 Years for 6 Node String

Number of Wavelengths Dropped per Node

= cumulative reliability of transfer nodes in string
=== cumulative reliability of repeater nodes in string
s === RESULT:network of 6 nodes
2 Xfer 3 Xfer 5 Xter 6 Xter
2 Rptr 3 Rptr 1 RPtr 0 Rptr
Il
4 6




3) 10 GbE Solution

An obvious simplification of an 8 x 1GbE DWDM solution is to omit multiplexing altogether and condense the wavelengths into one 10GbE stream. Presently Cisco Systems Inc. manufactures a switch comparable to that used in the DWDM solution, however it operates two 10G GBICs.


The major problem with 10G signaling over fiber is due to adverse affects of dispersion on the signal shape. The spectral line width of the DFB laser limits the modulation rate of the signal over long runs of dispersive media. More important signal chirp due to the very high speed electrical modulation of the laser results in edge phenomena, which result in signal distortion at long distances. This latter quantity is difficult to quantify, and is very dependent upon the driver circuits.


The ultimate solution to the aforementioned problem, is to omit electrical modulation of the laser, and to use optical modulation, which omits chirp altogether. The latter method was somewhat complex and expensive, employing Lithium Niobate crystals and a Mach-Zehnder interferometer. However recent developments by Intel have led to a silicon wafer based model, which promises compaction and cost effectiveness.

The tractable data rate as a function of dispersion, D, and distance, s can be given by:

Bitrate(Gb/s) x Length(km) = 1000/4Ds

4) DWDM System with Optical Modulator

As the optical fiber telecommunication technology is evolving very rapidly, a new technology which would be able to be used for scientific underwater cable networksin near future are emerging. Tokura et al[A] has proposed an optical modulator using a Raman amplifier for DWDM system. 

In the Raman modulator, the modulated driving current modulate the gain of the Raman amplifier, which modulate the career light.
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Fig.b shows the system configuration. In this system, all the light sources with highly stabilized wavelength are placed in terrestrial stations. In an underwater observation node, a corresponding wavelength is dropped from a (the first) optical fiber and return back to the terrestrial station through another (the second) optical fiber after being modulated by the Raman modulator. The same wavelength in the second optical fiber is also dropped at the same node, and is returned back to the another terrestrial terminal through the first optical fiber after being modulated. This means that even if the underwater cable is broken, all underwater observation nodes can continue data transmission with one of the terrestrial terminals.

The features of this system are

(a) Simple configuration

(b) The system consist of only field proven devices.
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(c) The wavelength stabilization systems including temperature controlling systems are located in terrestrial stations.

(d) Robustness against cable faults.

(e) About a hundred wavelength will be able to be used .

Although this is not COTS system, the system consists of COTS devices. These features implies high reliability and cost-effectiveness of the system.

One of the promising application of this system is ARENA. Fig.c shows an engineering model of ARENA[B] in which two horizontal trunk cable are placed at both side of a plate boundary, and these trunk cables are connected to plural terrestrial stations. This configuration having plural terrestrial stations enables step-by-step construction of the network corresponding to funding.

[image: image9.jpg]DWDM BRANCHING NODE for DEPLOYMENT AT MESH POINTS

Rcv East

|

YHON A%y

o)

—r
]
oo | £
s @
o
e | &
Ees et
g
nran” ~goEs) 5
e *[0 o € 3
=
el 1l —gEes
= I 7
&
H Hi
g
o
u
[
3
I g
Tx Ereg
North < | (x BH_
HSS
H-Eea—
7
|
= __, I
== i !
— i T o
8 ail) gy =
gl
e
Foes) @
o
coes | Q
Frage— 5
s — )
AEm —ge=a— 3
B ran._ R
e
Fees e KAE

Rcv West

Tx West

Science
Instrument




In the proposed data transmission system for ARENA, one or a few wavelengths are assigned to each node as shown in Fig.d. On each wavelength, an IP signal or a HDTV signal is transmitted. Backbone layer connects between the terrestrial terminals to increase the flexibility of the network. As laser diodes are placed in terrestrial terminals, it is easy to increase the number of wavelength without affecting any previously installed nodes. The system is robust against cable faults as the signal is transmitted to both directions.

We have done basic evaluation for optical modulator. It uses Raman amplifiers as modulators in underwater terminals. It would enable to use DWDM system in which all laser diodes for which accurate temperature control is needed are placed in land terminals. It would be a possible option for future network. I can briefly describe this method.

5) Summary

The characteristics of the four different options are summarized in the table below.

	TABLE III

COMPARISON OF OPTICAL DATA TRANSPORT OPTIONS

	Parameter
	CWDM
	DWDM
	10GbE

	Cost
	Low
	Moderate
	

	Distance
	80 km
	150 km
	

	Power Rqmts
	184 watts2
	300 watts1
	

	Thermal Output
	Same as above
	Same as above
	

	Complexity
	Simple
	Medium
	

	Reliability
	High
	Medium
	

	Size
	(2) 21x43x26

(2) 4.4x44.5x30
	(2) 4.4x44.5x30

(2) 48x9x18
	

	Notes
	1
	measured in lab using two Cisco 3750s and two NE optical frames

	
	2
	Estimated from specs: 24 W for 2x8 SFPs, 160W for 2xswitches

	
	3,4
	The additional optical-optical transponders make this solution more complex than the CWDM and introduce an additional point of failure in reliability calculations.


IV. NODE AND NETWORK RELIABILITY

The presently accepted link topology for NEPTUNE is constituted of a meshed network architecture, wherein each node contains a group of DWDM optical and GbE electrical devices to carry the primary network traffic. In order to further investigate the impact of meshing, and of redundancy of critical devices within the node, a study was performed to statistically determine the expectation of node availability to science, repair rate of node, and optimum node configuration. This study was divided into two phases as follows:

Node Reliability – Determine the best choice of OEO repeating wavelengths versus dropping wavelengths into the switching fabric

Network Reliability – Prove the adequacy of a meshed architecture, predict maintenance requirements and provide science users with reliability estimates.

1) Node Reliability

The Node Reliability phase is relevant to designing the internal node architecture. In this design DWDM channels pass through the node and can either be routed into the nodes electronic switching fabric, or passed through using only OEO repeating in the opto-electronic layer. In such a design it became apparent that the number of wavelengths to repeat with a node vs. the number to be add/dropped and routed via layer 3 algorithms must be determined. The cost, power consumption and reliability of the system are all functions of this number.

Certain assumptions were used:

· The data to be transported from an instrument to the shore can be aggregated over more than one wavelength using CISCO Ether channel algorithms. From the perspective of a reliability calculation this means that multiple redundant paths exist between nodes as the data is ported to the shore, and parallel probability calculations prevail.

· Efficiency of transport is not regarded and as such, reduced throughput due to malfunctioning parts is not considered a failure from sense of the reliability calculation.

· The intent of the calculation here, is to find the probability that:

· A particular instrument attached to a particular node will reach any exit path from the node.

· Incoming traffic to the node will find at least one exit path from the node

· The failure rate of a component in the node is not given as a function of time. Failure of a device here is defined as follows: Given a large number of duplicate devices d, the failure rate Fd is the number of failed devices divided by the total number after Y years of operation.

Fit rates, f, used in this for the study are shown below. The success rate is e-tfH where t is in years and H = 24x365.

	TABLE I

Subsea Component FIT rates used in the Node Reliability phase of the reliability study

	Component
	FIT Rate

	Optical Transmitter
	 460 x 10-9

	EDFA
	 100 x 10-9

	Packet Switch
	1000 x 10-9

	Optical Receiver
	 230 x 10-9


Two distinct NEPTUNE Node Types are identified in the reliability study:

2 way node type - This is a node, which has 2 external ports for data transfer to East and West. 8 instruments can be attached.

3 way node type - Also called a branching node, this is a node, which has 3 external ports for data transfer to East, West and North. 8 instruments can be attached. 

For each of these node, three different modes of operation are defined:

Instrument mode - Node transfers data from an instrument to the East or West external port.

Transfer mode - The node receives the instrument data from an adjacent node, passes it to the switch layer, and then transfers it to the next node.

Repeat mode - The node receives the instrument data from an adjacent node and than transfers it to the next node, without first sending it through the switches. All processing is done by the optical layer including the transponders. The data is OEO repeated.

The present NEPTUNE node design consists of a Network Electronics Optical switch, a Bookham EDFA, and a Cisco Systems electrical GbE switch. This assembly is duplicated in the node for redundancy. Using the above design considerations a mathematical model was written for the node internals calculating the failure rate for the highly parallelized architecture. This model calculated the number of node-drops vs. pass-through as a function of reliability. The result is shown graphically below:

Based on the above graph, the decision was made to drop all 8 DWDM channels in each node. The inherent benefits of this are:

· The most flexible routing capability during an outage providing the maximum number of alternate routes

· The most flexibility when tuning providing the maximum number of possible paths for balancing traffic

· The best internode latency figure- direct node to node communications over Layer2

· Full Bandwidth Access to the 8G Backbone

2) Network Reliability

The Network Reliability phase is relevant to designing the mesh and routing algorithms of the network architecture. In this design all of the DWDM channels pass through the network from node to node. At strategic points, 3-way backbone branching nodes are inserted, providing alternate data paths, giving the architecture its reliability.

The objectives of the Network Reliability Study were:

· Scientist: Concerned with number of paths available form equipment to shore as a function of time.

· Chart Available Paths at Each Node

· Systems Engineering and Management: Concerned with number of ship visits per year to keep all devices in nodes running

· Block Reliability Chart for Whole System
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Design Engineer: Concerned with reliability of individual parts over time

· Plot Device Reliability for a Node

The Network Reliability study is performed by first assigning each major device in the node a reliability value. Each device within the node is given a state of failed or not-failed using a Monte Carlo algorithm. The node, as a complete entity, is either capable or not-capable of transferring instrument traffic based upon the failure state of the devices. 

This Monte Carlo program was run using the FIT rates for the devices in the nodes. The outcomes are shown in the two plots below.


The first plot above demonstrates that if the nodes are not periodically repaired as their internal devices fail, eventually the node will completely fail to transfer traffic after 13 years. Due to the realistic likelihood of ship visits to deploy equipment, coupled with an expected cyclic maintenance program at each node, this is an acceptable risk.

The second plot demonstrates that regardless of complete failures of an individual node the remaining nodes will continue to have a portal to transmit their traffic to the shore after 15 years. After 15 years, all 26 nodes on the x-axis have at least 5 remaining paths to the shore.

The conclusion of this study is that the deployment of commercially terrestrial devces in a redundant and meshed architecture provides the oceanographic community with a flexible, template-able, and cost effective technique for use in regional cabled observatories.

V. ARENA AND NEPTUNE DESIGN STATUS

[Kenichi, Need to expand for ARENA

The present design status for NEPTUNE is largely correlated with the program on the aforementioned MARS project, which is a single, 3 channel NEPTUNE node expected to be deployed off the California coast next year. Additional work unique to NEPTUNE's mesh and reliability architecture has been completed as well, including the network reliability study mentioned in this paper, the conceptual design of mesh branching units, and the power system design which insures the safety of adjacent nodes when a single node encounters a power failure or ground fault.


The key issues researched in the laboratory at this time for MARS were thermal properties and optical transport properties using the same suite of devices already mentioned for NEPTUNE including Nortel EDFAs, Network Electronics optical switches, and CISCO electrical routers.


In the thermal area the power consumption of all the MARS data communications equipment was measured under real data loads. These power values were used to inject heat using heating elements into a comparable node enclosure and determine the resulting temperature rise. These measurements were done in air and will be completed in a water bath soon. In addition the use of Fluorinert cooling fluid was investigated. It was determined that the CISCO routers will require immersion in the Fluorinert, while the NE optical switches and EDFAs run cooler and can be placed in a dry air section of the node enclosure. (Fluorinert filled the air gap found in GBIC and SPF optics hence it could not be used here). We expect that heat sinking will be advisable for the NEPTUNE node with its full 8 channel capacity. The first experimental estimate of the thermal conditions is shown in the graph below. The results shown in red are tests which were repeated adding 4 cooling fans to the node. It is apparent that temperatures less than 35 degrees are achievable with a power injection of 90 watts, which is typical for this section of the node, based upon electrical power measurements. Submersion of the node in water should bring the temperatures well below 30 degrees. The use of fans is well worth investigating should thermal issues become a problem.There are presently on the market, small cooling fans using sintered bearing which have a MTBF on the order of 300,000 hours.
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At this time, the ability of the chosen equipment to operate at the accepted GbE error rate of 10-12 has been proven over 100 km runs of SMF28E fiber. Runs were done for 24 hours using both a booster EDFA and a pre-amp EDFA. More work is in progress to test past distances of 150km, which will cover all NEPTUNE distances excepting one shore connection. For these tests we will have the option of using both a booster amplifier and a pre-amplifier in concert. Additionally fiber of lower dispersion than SMF28E can be used for longer runs.
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The above work completes the proof of concept for the primary data communications of the NEPTUNE system. Remaining major issues are improving a "Y" cable science connector to allow redundancy to the routers, and asserting the reliability of wet optical connectors for node deployment. 

It is understandable that the US and Japan efforts have adopted two different approaches for the design of NEPTUNE and ARENA observatories, respectively. 

One factor which drives the different design philosophies is that NEPTUNE engineering is being for the most part done in academic institutions, with plans to perform the fabrication and installation under industrial contract. The US feels that this approach will make it more probable that the resulting observatory will include the unique features required by the scientific community rather than compromise features in favor of industries preference for building systems closer to the design of existing systems.

The Arena observatory effort, on the other hand, favors a closer relationship with industry during the design phase. They feel that [Need some words from Kenichi here]
The followings are my suggestion.

It is clear that there are some technical options in communication systems for scientific underwater cable network. The most desirable option would depend on the network configurarion, its scale, its scientific objectives and state of the art when the development is inaugurated.

In NEPTUNE, the optical GbE over DWDM system was selected for laboratory test. It is interesting that in ARENA, IP over DWDM system was also proposed [B]. 

As ARENA project is still under feasibility study stage, and the system has not yet fixed. DWDM with Raman modulator is just one of the options. As the technology is evolving very rapidly, it will adopt the most attractive technology when the design will have to be fixed.

Although the NEPTUNE and ARINA has almost the same scientific objective and share the common basic requirements, their priorities are slightly different. In ARENA, seismic research has greater importance, as there are many catastrophic earthquakes in Japan. That means that the system should keep working when big earthquakes hit the network The system shoule be robust against damages. These differences might affect the detailed design of the system.

.Please add some words or revise the words.
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Fig.b COnfiguration of DWDM with Raman dodulators
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Fig.c Engineering model of underwater cable netwrok for ARENA
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Fig.d Proposed wavelength assignment for ARENA system





Comments:  Please delete from the paper





I think it is not important that NEPTUNE engineering was done for most part in academic institutions and ARENA engineering was done in IEEE OES in which most researchers are from private business. The feasibility study for ARENA was done based upon the basic requirement described in the paper, and do not have preference to the design of existing systems. I also would like to point out that the IP over DWDM system was also prefered for ARENA project. The only difference was that in ARENA, 100Base system was proposed, instead of Giga Ether. But it was two years ago, and the situation might have been changed.


I think the most desirable option would depend on the network configurarion (or scale), its scientific objectives and state of the art when the development is inaugurated. Although the NEPTUNE and ARINA has the same scientific prospect, i.e. multidisciplinary objectives, and share the common basic requirements, their priority might be slightly different. In ARENA, seismic research has greater importance, as there are many catastrophic earthquakes in Japan, which means that the system should keep working when big earthquakes occur. The system shoule be robust against damages. The underwater devices are required to be deployed up to 6,000 meters in depth across the plate boudaries, which means that the underwater devices should be small and light so that it can be handled by research vessels and/or cable ships. These differences would affect the detailed design of the system.


In ARENA project, as the funding is not yet obtained, it is still under feasibility study, and the system is not yet fixed. DWDM with Raman modulator is just one of options. As the technology is evolving very rapidly, it will adopt the most attractive technology when we will have to fix the design. 
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