LV – Low voltage.  Refers to the power regulation,switching components in the wet (fluorinert) section of the LV pressure vessel, as well as that pressure vessel as a whole.  Includes the 400V and 48V power supplies for the science payloads, as well as the hotel power.

MV – Medium voltage.  Refers to the components which handles the 10kV coming from the cable (via the cable termination xxx), and the pressure vessel in which they are housed.

DCS –
OOB, OBC – Out of Band/Out-of-Band Controller.

