CIMT FREEWAVE RADIO CONFIGURATION TABLE

	Name /

Serial Number
	Modem Mode
	Baud Rate
	Call Book
	Frequency Key
	RF Data Rate /

RF Power

	Mooring Primary

915-3373
	(1)   Point to Point Slave
	57600
	(0)     915-4162

(1)     915-4161

(2)     903-7091
	12
	3 /

10

	Shore

Primary

915-4162
	(0)   Point to Point Master
	57,600
	(0)     915-3373

(1)     915-3374

Calls 00
	12
	3 / 

10

	Mooring

Secondary

915-3374
	(1)   Point to Point Slave
	38,400
	
	13
	3 /

1

	Shore Secondary
	(0)   Point to Point Master
	57,600
	(0)     915-3373

(1)     915-3374

Calls 00
	12
	3 /

10

	Operations / Spare
	(0)   Point to Point Master
	38,400
	(0)    915-3374

Calls 00
	13
	3 /

1

	
	
	
	
	
	


Note:
Table date Monday, May 17, 2004

The Shore Secondary is configured as a spare for use in the Cupola in the event that the Shore Primary malfunctions.

The Operations / Spare radio will be configured to communicate from the Pt. Sur to the Mooring Primary radio.  This spare radio could later be used on the shore or mooring.

The Mooring Secondary is the mooring spare for now.  It is installed in a radio housing.

The Can color scheme is as follows:

Primary radio pair
Green

Secondary radio pair
Yellow

Operations

Red

The colors apply to the current configuration and not the physical addresses.

