Revision History

05/05/04 - created (klh)

05/10/04 - added puck/jar, dpa channels (klh)

05/13/04 – updated with changes to wiring of section 3B

05/17/04 – corrected port numbers for secondary/primary radio

	Instrument
	SSDS Device ID
	Pie Connector
	DPA Port
	DPA Board/Chan
	Puck/Jar
	Sample Interval (s)

	Metsys
	1321
	1C
	1
	0/1
	p
	600

	ADCP
	1267
	2E
	6
	3/0
	p
	600

	Spare
	-
	2C
	4
	2/0
	-
	-

	Spare
	-
	3B
	0
	0/0
	-
	-

	Serial CTD
	1314
	3E
	10
	5/0
	p
	600

	Inductive CTD 10m
	1318
	-
	-
	-
	-
	600

	Inductive CTD 20m
	1317
	-
	-
	-
	-
	600

	Inductive CTD 40m
	1316
	-
	-
	-
	-
	600

	Inductive CTD 60m
	1315
	-
	-
	-
	-
	600

	Inductive Modem
	1319
	2F
	7
	3/1
	j
	600

	Inductive Coupler
	-
	-
	-
	-
	-
	-

	Nitrate
	1268
	3F
	11
	5/1
	p
	600

	CO2
	1275?
	-
	-
	-
	-
	600

	Radiometers
	1326
	-
	-
	-
	-
	600

	Radiometers
	1323
	-
	-
	-
	-
	600

	Radiometers
	1312
	2D
	5
	2/1
	p
	600

	Radiometers
	1324
	-
	-
	-
	-
	600

	Radiometers
	1325
	-
	-
	-
	-
	600

	Fluorometer
	1279
	3D
	9
	4/1
	p
	600

	Backscatter
	1301
	3C
	8
	4/0
	p
	600

	Locator
	1302 (GPS) 1303(Orbcomm)
	-
	-
	-
	-
	3600

	GPS
	1313
	1D
	2
	1/0
	p
	600

	Primary Radio
	-
	2A,2B
	-
	-
	-
	-

	Secondary Radio
	-
	3A
	-
	-
	-
	-

	Shore Radio
	-
	-
	-
	-
	-
	-

	Power System Data
	1322
	1E
	3
	1/1
	j
	-

	MSP430
	1300
	-
	-
	-
	j
	-

	Compass
	-
	-
	-
	-
	-
	-

	Power
	-
	1F
	-
	-
	-
	-

	MMC Node
	1299
	-
	-
	-
	-
	-

	ethernet
	-
	-
	-
	-
	-
	-

	console
	-
	1A
	-
	-
	-
	-

	pager reset
	-
	1B
	-
	-
	-
	-


