Re-Work Instructions for SideARM Revision 4.10

ECO #1, Revision 1, February 3, 2004

1.
Connect pin 13 of J5 to pin 8 of J6 on the topside of the PCB.

2. Connect C10 pin 1 (+3.3V side) to U3 pin 5.  Pin 1 of C10 is closest to R21 on the bottom side of the PCB.


3. 
Connect pin 62 and pin 63 of U21 (MSP430).  A solder blob or blue wire can be used.


4.
Lift pin 2 of U1.

Lift pin 8 of U1.

Connect pad 2 of U1 to pin 8 of U1.

Connect pad 8 of U1 to pin 2 of U1.

