SideARMTest Punch List
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Serial #:______________
1.
Boots Linux





Pass
Fail
Date:

2.
Ethernet MAC Address Set



Pass
Fail
Date:


3.
Ping another system




Pass
Fail
Date:

4.
Create file on Compact Flash



Pass
Fail
Date:

5.
Read file on Compact Flash



Pass
Fail
Date:

6.
Append to file on Compact Flash



Pass
Fail
Date:

7.
Delete file on Compact Flash



Pass
Fail
Date:


8.
UART   0 Internal Loop Back



Pass
Fail
Date:

9.
UART   1 Internal Loop Back



Pass
Fail
Date:

10.
UART   2 Internal Loop Back



Pass
Fail
Date:

11.
UART   3 Internal Loop Back



Pass
Fail
Date:

12.
UART   4 Internal Loop Back



Pass
Fail
Date:

13.
UART   5 Internal Loop Back



Pass
Fail
Date:

14.
UART   6 Internal Loop Back



Pass
Fail
Date:

15.
UART   7 Internal Loop Back



Pass
Fail
Date:

16.
UART   8 Internal Loop Back



Pass
Fail
Date:

17.
UART   9 Internal Loop Back



Pass
Fail
Date:

18.
UART 10 Internal Loop Back



Pass
Fail
Date:

19.
UART 11 Internal Loop Back



Pass
Fail
Date:

20.
Long Range Radio Loop Back



Pass
Fail
Date:

21.
Long Range Radio Power Switch



Pass
Fail
Date:

22.
Short Range Radio Loop Back



Pass
Fail
Date:

23.
Short Range Radio Power Switch



Pass
Faill
Date:

24.
Temperature Sensor 




Pass
Fail
Date:

25.
Humidity Sensor





Pass
Fail
Date:

26.
Pressure
 Sensor





Pass
Fail
Date:

27.
High Side Ground Fault Current



Pass
Fail
Date:

28.
Low Side Ground Fault Current



Pass
Fail
Date:

29.
High Side Ground Fault Injector



Pass
Fail
Date:

30.
Low Side Ground Fault Injector



Pass
Fail
Date:

31.
Set Ricoh Clock



No SW

Pass
Fail
Date:

32.
Read Ricoh Clock


No SW

Pass
Fail
Date:

33.
Ricoh Clock correct after power cycle
No SW

Pass
Fail
Date:

34.
KVH UART Loop Back




Pass
Fail
Date:

35.
KVH Analog Port




Pass
Fail
Date:

36.
KVH Power Switch




Pass
Fail
Date:

37.
Wake Up from internal RTC

No SW

Pass
Fail
Date:

38.
Wake Up from Ricoh RTC

No SW

Pass
Fail
Date:

