1002892-BPB1B README_FAB.TXT

Design Contact: John Zsori, CID+ - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
Cell:    408.391.6656
email:   john_zsori@pacbell.net

Client: MBARI
7700 Sandholdt Road
Moss Landing, CA  95039
Denis Klimov - 831.775.1700


Fabrication data included in 1002892-BPB1B_CAM.ZIP:

                PowerPCB Gerber Files (RS-274-X Format)
      
1002892-BPB1B-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Primary (Top) Side)
1002892-BPB1B-TS.PHO     Primary Silkscreen (Top)
1002892-BPB1B-BS.PHO     Secondary Silkscreen (Bottom)  
1002892-BPB1B-TM.PHO     Primary Solder Mask (Top)
1002892-BPB1B-BM.PHO     Secondary Solder Mask (Bottom)
1002892-BPB1B-TP.PHO     Primary Paste Mask (Top)
01002892-BPB1B-BP.PHO    Secondary Paste Mask (Bottom)
1002892-BPB1B-DD.PHO     Drill Drawing
1002892-BPB1B-DD.PDF     Drill Drawing in Adobe format

	Drill Files

1002892-BPB1B-NC.DRL     NC Drill

                Netlist

1002892-BPB1B-IPC.NET    IPC-D-356 Format Netlist (See Note 2 and 3)

Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask 
size to your specific manufacturing tolerances while maintaining maximum web.

2. Compare the IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.

3. Note that short circuits across obround pads and holes of PA1 and PA2 are by design.
