1002605REV2 README_FAB.TXT

Design Contact: John Zsori - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
Mobile:  408.391.6656
email:   jzsori@pacbell.net

PLEASE REFER ALL PCB DESIGN RELATED ISSUES TO JOHN ZSORI

Client: MBARI
7700 Sandholdt Road
Moss Landing, CA  95039
Wayne Radochonski - 831.775.1700


Fabrication data included in 1002605REV2_CAM.ZIP:

                PowerPCB V5.0.1 Gerber Files (RS-274-X Format)
      
1002605REV2-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Top Side)
1002605REV2-ST.PHO     Silkscreen Top
1002605REV2-SB.PHO     Silkscreen Bottom  
1002605REV2-MT.PHO     Solder Mask Top
1002605REV2-MB.PHO     Solder Mask Bottom
1002605REV2-PT.PHO     Paste Mask Top
1002605REV2-PB.PHO     Paste Mask Bottom
1002605REV2-DD.PHO     Drill Drawing
1002605REV2-DD.PDF     Drill Drawing in Adobe format


                Drill Files

1002605REV2-NC.DRL     NC Drill


                 Netlist

1002605REV2-IPC.NET    IPC-D-356 Format Netlist (See Note 2)


Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask 
size to your specific manufacturing tolerances.

2. Compare the IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.
