1002606_2 README_FAB.TXT

Design Contact: John Zsori - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
Mobile:  408.391.6656
email:   jzsori@pacbell.net

Fabrication data included in 1002606_2_CAM.ZIP:

                PowerPCB V5.0.1 Gerber Files (RS-274-X Format)
      
1002606_2-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Top Side)
1002606_2-ST.PHO     Silkscreen Top
1002606_2-SB.PHO     Silkscreen Bottom
1002606_2-MT.PHO     Solder Mask Top
1002606_2-MB.PHO     Solder Mask Bottom
1002606_2-PT.PHO     Paste Mask Top
1002606_2-PB.PHO     Paste Mask Bottom
1002606_2-DD.PHO     Drill Drawing

                Fabrication Drawings

1002606_2-DD.PDF     Drill Drawing in Adobe Format


		 Drill Files

1002606_2-NC.DRL     NC Drill File
1002606_2-NC.REP     NC Drill Report (Sizes & Quantities)
1002606_2-NC.LST     NC Drill Sizes & Coordinates


                Netlist

1002606_2-IPC.NET    IPC-D-356 Format Netlist (See Note 2)


		Misc.

1002606_2.PDF	PDF Gerber Verify Plots


Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask 
size to your specific manufacturing tolerances.

2. Compare the IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.
