1002604_1 README_FAB.TXT

Design Contact: John Zsori - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
email:   jzsori@pacbell.net

REFER ALL PCB DESIGN RELATED ISSUES TO JOHN ZSORI

Client: MBARI
7700 Sandholdt Road
Moss Landing, CA  95039
Wayne Radochonski - 831.775.1700


Fabrication data included in 1002604_1-CAM.ZIP:

                PowerPCB V5.0.1 Gerber Files (RS-274-X Format)
      
1002604_1-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Top Side)
1002604_1-ST.PHO     Silkscreen Top
1002604_1-SB.PHO     Silkscreen Bottom  
1002604_1-MT.PHO     Solder Mask Top
1002604_1-MB.PHO     Solder Mask Bottom
1002604_1-DD.PHO     Drill Drawing
1002604_1-DD.PDF     Drill Drawing (PDF Format)


		 Drill Files

1002604_1-NC.DRL     NC Drill File THRU VIA
1002604_1-NC1-5.DRL  NC Drill Blind VIA 1-5
1002604_1-NC8-12.DRL NC Drill Blind VIA 8-12 


                Netlist

1002604_1-IPC.NET    IPC-D-356 Format Netlist (See Note 3)


Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask 
size to your specific manufacturing tolerances.

2. Teardrop may be added to all trace to pad entries as required. Insure that the 
final result passes all DRC spacing requirements. 

3. Compare the IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.
